# Heart Rate Channel example - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Heart Rate Channel example**

## Example Device: Heart Rate Channel example

| |
| :--- |
| *Page standards status:*[Informative](http://hl7.org/fhir/R4/versions.html#std-process) |

Profile: [Channel Device profile](StructureDefinition-ChannelDevice.md)

**status**: Active

**type**: MDC_DEV_CARD_RATE_CHAN

**parent**: [Device: status = active; type = MDC_DEV_ECG_VMD](Device-ECGVmdDevice.md)



## Resource Content

```json
{
  "resourceType" : "Device",
  "id" : "HeartRateChannelDevice",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/uv/pocd/StructureDefinition/ChannelDevice"]
  },
  "status" : "active",
  "type" : {
    "coding" : [{
      "system" : "urn:iso:std:iso:11073:10101",
      "code" : "70739",
      "display" : "MDC_DEV_CARD_RATE_CHAN"
    }]
  },
  "parent" : {
    "reference" : "Device/ECGVmdDevice"
  }
}

```
