Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example Device: Patient Monitor MDS example

Page standards status: Informative

Profile: MDS Device profile

> Approved Jurisdictions extension

> - approvedJurisdiction: United States of America (the)

Operator extension: Practitioner Alice B. Careful

Operating hours extension: 8760

Operating cycles extension: 156

Operating mode extension: Dmo

identifier: `urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680`/01-23-45-67-89-AB-CD-EF

### UdiCarriers

- | DeviceIdentifier | CarrierHRF
* | 00012345678905 | (01)00012345678905(21)123456

status: Active

manufacturer: MyCompany

serialNumber: 123456

### DeviceNames

- | Name | Type
* | MyPhysioMonitor | Model name

modelNumber: PM1

type: Patient Monitor

patient: John Doe Male, DoB: 1967-05-04 ( Medical record number)

location: Location Bed 42