Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## Example DeviceMetric: Heart Rate Numeric metric example

Page standards status: Informative

Profile: Numeric DeviceMetric profile

> Relation extension

> - kind: DCE
> - entries: DeviceMetric: extension = 0.001,25 mm/s; type = MDC_ECG_ELEC_POTL; unit = MDC_DIM_MILLI_VOLT; operationalStatus = on; color = green; category = measurement

> Technical range extension

> - lowerLimit: 0
> - upperLimit: 200
> - stepWidth: 1
> - relativeAccuracy: 0.01
> - absoluteAccuracy: 0.01

> Reference range extension

> - type: Alarm limits
> - low: 40 bpm (Details: unknown code264864 = 'MDC_DIM_BEAT_PER_MIN')
> - high: 180 bpm (Details: MDC Nomenclature code264864 = 'MDC_DIM_BEAT_PER_MIN')

type: HR

unit: bpm

source: Device: extension = ,->Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS

parent: Device: status = active; type = MDC_DEV_CARD_RATE_CHAN

operationalStatus: On

color: Color Green

category: Measurement