## Intersection of http://hl7.org/fhir/uv/pocd/StructureDefinition/VmdDevice and http://hl7.org/fhir/uv/pocd/StructureDefinition/VmdDevice

This is the set of resources that conform to both VMD Device profile (http://hl7.org/fhir/uv/pocd/StructureDefinition/VmdDevice) and VMD Device profile (http://hl7.org/fhir/uv/pocd/StructureDefinition/VmdDevice).

### Structure

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* |  | Item used in healthcare
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Extension
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
extension |  | 0..* | Extension | Additional content defined by implementations
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: ?? (required): Identifies the purpose for this identifier, if known .
type | Σ | 0..1 | CodeableConcept | Description of identifier Binding: ?? (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
system | Σ | 0..1 | uri | The namespace for the identifier value Example General: http://www.acme.com/identifiers/patient
value | Σ | 0..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | S Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered.
status | ?!S Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device.
statusReason | S | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer | S | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber | S | 0..1 | string | Serial number assigned by the manufacturer
deviceName | S | 0..* | BackboneElement | The name of the device as given by the manufacturer
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by.
modelNumber | S | 0..1 | string | The model number for the device
partNumber | S | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: ?? (extensible)
extension |  | 0..* | Extension | Additional content defined by implementations
coding | Σ | 0..* | Coding | Code defined by a terminology system
extension |  | 0..* | Extension | Additional content defined by implementations
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version | S | 0..* | BackboneElement | The actual design of the device or software version running on the device
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
extension |  | 0..* | Extension | Additional content defined by implementations
coding | Σ | 0..* | Coding | Code defined by a terminology system
extension |  | 0..* | Extension | Additional content defined by implementations
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | S Σ | 0..* | CodeableConcept | Safety Characteristics of Device
extension |  | 0..* | Extension | Additional content defined by implementations
coding | Σ | 0..* | Coding | Code defined by a terminology system
extension |  | 0..* | Extension | Additional content defined by implementations
system | Σ | 0..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 0..1 | code | Symbol in syntax defined by the system Binding: ?? (required): Safety classification
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
parent | S | 1..1 | Reference(MDS Device profile | #sd+11-MdsDevice-MdsDevice) | The parent device
Documentation for this format