Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Heart Rate Numeric metric example - TTL Representation

Page standards status: Informative

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdf: <http://www.w3.org/1999/02/22-rdf-syntax-ns#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:DeviceMetric ;
      fhir:nodeRole fhir:treeRoot ;
      fhir:id [ fhir:v "HeartRateNumericDeviceMetric"] ; #
      fhir:meta [
        ( fhir:profile [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric>     ] )
      ] ; #
      fhir:text [
    fhir:status [ fhir:v "extensions" ] ;
    fhir:div [ fhir:v "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p class=\"res-header-id\"><b>Generated Narrative: DeviceMetric HeartRateNumericDeviceMetric</b></p><a name=\"HeartRateNumericDeviceMetric\"> </a><a name=\"hcHeartRateNumericDeviceMetric\"> </a><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\"/><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-NumericDeviceMetric.html\">Numeric DeviceMetric profile</a></p></div><blockquote><p><b>Relation extension</b></p><ul><li>kind: DCE</li><li>entries: <a href=\"DeviceMetric-ECGSampleArrayDeviceMetric.html\">DeviceMetric: extension = 0.001,25 mm/s; type = MDC_ECG_ELEC_POTL; unit = MDC_DIM_MILLI_VOLT; operationalStatus = on; color = green; category = measurement</a></li></ul></blockquote><blockquote><p><b>Technical range extension</b></p><ul><li>lowerLimit: 0</li><li>upperLimit: 200</li><li>stepWidth: 1</li><li>relativeAccuracy: 0.01</li><li>absoluteAccuracy: 0.01</li></ul></blockquote><blockquote><p><b>Reference range extension</b></p><ul><li>type: <span title=\"Codes:{http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type alarm-limits}\">Alarm limits</span></li><li>low: 40 bpm<span style=\"background: LightGoldenRodYellow\"> (Details: unknown  code264864 = 'MDC_DIM_BEAT_PER_MIN')</span></li><li>high: 180 bpm<span style=\"background: LightGoldenRodYellow\"> (Details: MDC Nomenclature  code264864 = 'MDC_DIM_BEAT_PER_MIN')</span></li></ul></blockquote><p><b>type</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 147842}\">HR</span></p><p><b>unit</b>: <span title=\"Codes:{urn:iso:std:iso:11073:10101 264864}\">bpm</span></p><p><b>source</b>: <a href=\"Device-PhysioMonitorMdsDevice.html\">Device: extension = ,-&gt;Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS</a></p><p><b>parent</b>: <a href=\"Device-HeartRateChannelDevice.html\">Device: status = active; type = MDC_DEV_CARD_RATE_CHAN</a></p><p><b>operationalStatus</b>: On</p><p><b>color</b>: Color Green</p><p><b>category</b>: Measurement</p></div>"^^rdf:XMLLiteral ]
      ] ; #
      fhir:extension ( [
    fhir:url [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/relation"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/StructureDefinition/relation>     ] ;
        ( fhir:extension [
    fhir:url [
    fhir:v "kind"^^xsd:anyURI ;
    fhir:l fhir:kind       ] ;
    fhir:value [
    a fhir:Code ;
    fhir:v "DCE"       ]     ] [
    fhir:url [
    fhir:v "entries"^^xsd:anyURI ;
    fhir:l fhir:entries       ] ;
    fhir:value [
    a fhir:Reference ;
    fhir:l fhir:DeviceMetric/ECGSampleArrayDeviceMetric ;
    fhir:reference [ fhir:v "DeviceMetric/ECGSampleArrayDeviceMetric" ]       ]     ] )
      ] [
    fhir:url [
    fhir:v "http://hl7.org/fhir/uv/pocd/StructureDefinition/technical-range"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/StructureDefinition/technical-range>     ] ;
        ( fhir:extension [
    fhir:url [
    fhir:v "lowerLimit"^^xsd:anyURI ;
    fhir:l fhir:lowerLimit       ] ;
    fhir:value [
    a fhir:Decimal ;
    fhir:v "0"^^xsd:decimal       ]     ] [
    fhir:url [
    fhir:v "upperLimit"^^xsd:anyURI ;
    fhir:l fhir:upperLimit       ] ;
    fhir:value [
    a fhir:Decimal ;
    fhir:v "200"^^xsd:decimal       ]     ] [
    fhir:url [
    fhir:v "stepWidth"^^xsd:anyURI ;
    fhir:l fhir:stepWidth       ] ;
    fhir:value [
    a fhir:Decimal ;
    fhir:v "1"^^xsd:decimal       ]     ] [
    fhir:url [
    fhir:v "relativeAccuracy"^^xsd:anyURI ;
    fhir:l fhir:relativeAccuracy       ] ;
    fhir:value [
    a fhir:Decimal ;
    fhir:v 0.01       ]     ] [
    fhir:url [
    fhir:v "absoluteAccuracy"^^xsd:anyURI ;
    fhir:l fhir:absoluteAccuracy       ] ;
    fhir:value [
    a fhir:Decimal ;
    fhir:v 0.01       ]     ] )
      ] [
    fhir:url [
    fhir:v "http://hl7.org/fhir/StructureDefinition/reference-range"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/StructureDefinition/reference-range>     ] ;
        ( fhir:extension [
    fhir:url [
    fhir:v "type"^^xsd:anyURI ;
    fhir:l fhir:type       ] ;
    fhir:value [
    a fhir:CodeableConcept ;
            ( fhir:coding [
    fhir:system [
    fhir:v "http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type"^^xsd:anyURI ;
    fhir:l <http://hl7.org/fhir/uv/pocd/CodeSystem/reference-range-type>           ] ;
    fhir:code [ fhir:v "alarm-limits" ] ;
    fhir:display [ fhir:v "Alarm limits" ]         ] )       ]     ] [
    fhir:url [
    fhir:v "low"^^xsd:anyURI ;
    fhir:l fhir:low       ] ;
    fhir:value [
    a fhir:Quantity ;
    fhir:value [ fhir:v "40"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "bpm" ] ;
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>         ] ;
    fhir:code [ fhir:v "264864" ]       ]     ] [
    fhir:url [
    fhir:v "high"^^xsd:anyURI ;
    fhir:l fhir:high       ] ;
    fhir:value [
    a fhir:Quantity ;
    fhir:value [ fhir:v "180"^^xsd:decimal ] ;
    fhir:unit [ fhir:v "bpm" ] ;
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>         ] ;
    fhir:code [ fhir:v "264864" ]       ]     ] )
      ] ) ; #
      fhir:type [
        ( fhir:coding [
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>       ] ;
    fhir:code [ fhir:v "147842" ] ;
    fhir:display [ fhir:v "MDC_ECG_HEART_RATE" ]     ] ) ;
    fhir:text [ fhir:v "HR" ]
      ] ; #
      fhir:unit [
        ( fhir:coding [
    fhir:system [
    fhir:v "urn:iso:std:iso:11073:10101"^^xsd:anyURI ;
    fhir:l <urn:iso:std:iso:11073:10101>       ] ;
    fhir:code [ fhir:v "264864" ] ;
    fhir:display [ fhir:v "MDC_DIM_BEAT_PER_MIN" ]     ] ) ;
    fhir:text [ fhir:v "bpm" ]
      ] ; #
      fhir:source [
    fhir:l fhir:Device/PhysioMonitorMdsDevice ;
    fhir:reference [ fhir:v "Device/PhysioMonitorMdsDevice" ]
      ] ; #
      fhir:parent [
    fhir:l fhir:Device/HeartRateChannelDevice ;
    fhir:reference [ fhir:v "Device/HeartRateChannelDevice" ]
      ] ; #
      fhir:operationalStatus [ fhir:v "on"] ; #
      fhir:color [ fhir:v "green"] ; #
      fhir:category [ fhir:v "measurement"] . #