# Operating mode code system - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Operating mode code system**

## CodeSystem: Operating mode code system 

| | | |
| :--- | :--- | :--- |
| *Official URL*:http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode | *Version*:1.0.0 | |
| * Standards status: *[Trial-use](http://hl7.org/fhir/R4/versions.html#std-process) | [Maturity Level](http://hl7.org/fhir/versions.html#maturity): 2 | *Computable Name*:OperatingMode |

 
CodeSystem for IEEE 11073-10207 MdsState/OperatingMode 

 This Code system is referenced in the content logical definition of the following value sets: 

* [OperatingMode](ValueSet-operating-mode.md)



## Resource Content

```json
{
  "resourceType" : "CodeSystem",
  "id" : "operating-mode",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/StructureDefinition/shareablecodesystem"]
  },
  "extension" : [{
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg",
    "valueCode" : "dev"
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm",
    "valueInteger" : 2,
    "_valueInteger" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status",
    "valueCode" : "trial-use",
    "_valueCode" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  }],
  "url" : "http://hl7.org/fhir/uv/pocd/CodeSystem/operating-mode",
  "version" : "1.0.0",
  "name" : "OperatingMode",
  "title" : "Operating mode",
  "status" : "active",
  "experimental" : false,
  "date" : "2020-05-12",
  "publisher" : "HL7 International / Devices",
  "contact" : [{
    "telecom" : [{
      "system" : "url",
      "value" : "http://www.hl7.org/Special/committees/healthcaredevices"
    }]
  }],
  "description" : "CodeSystem for IEEE 11073-10207 MdsState/OperatingMode",
  "jurisdiction" : [{
    "coding" : [{
      "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
      "code" : "001"
    }]
  }],
  "caseSensitive" : false,
  "content" : "complete",
  "concept" : [{
    "code" : "Nml",
    "display" : "Normal",
    "definition" : "The POC MEDICAL DEVICE operates in a mode that supports the fulfillment of its clinical functions."
  },
  {
    "code" : "Dmo",
    "display" : "Demo",
    "definition" : "The POC MEDICAL DEVICE operates in a mode that is intended for demonstration purposes only. Arbitrary values are generated."
  },
  {
    "code" : "Srv",
    "display" : "Service",
    "definition" : "The POC MEDICAL DEVICE operates in a mode that is intended for services purposes only."
  },
  {
    "code" : "Mtn",
    "display" : "Maintenance",
    "definition" : "Maintenance. The POC MEDICAL DEVICE operates in a mode that is intended for maintenance purposes only."
  }]
}

```
