Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Heart Rate Numeric observation example - XML Representation

Page standards status: Informative

Raw xml | Download

    <Observation xmlns="http://hl7.org/fhir">
      <id value="HeartRateNumericObservation"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericObservation"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: Observation HeartRateNumericObservation</b></p><a name="HeartRateNumericObservation"> </a><a name="hcHeartRateNumericObservation"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-NumericObservation.html">Numeric Observation profile</a></p></div><p><b>status</b>: Final</p><p><b>category</b>: <span title="Codes:{http://terminology.hl7.org/CodeSystem/observation-category vital-signs}">Vital Signs</span></p><p><b>code</b>: <span title="Codes:{http://loinc.org 8867-4}, {urn:iso:std:iso:11073:10101 147842}">Heart rate</span></p><p><b>subject</b>: <a href="Patient-SomePatient.html">John Doe  Male, DoB: 1967-05-04 ( Medical record number)</a></p><p><b>effective</b>: 2021-07-09 11:33:24+0200</p><p><b>value</b>: 60 bpm<span style="background: LightGoldenRodYellow"> (Details: UCUM  code/min = '/min')</span></p><p><b>device</b>: <a href="DeviceMetric-HeartRateNumericDeviceMetric.html">DeviceMetric: extension = ,,; type = MDC_ECG_HEART_RATE; unit = MDC_DIM_BEAT_PER_MIN; operationalStatus = on; color = green; category = measurement</a></p></div>
      </text>
      <status value="final"/>
      <category>
        <coding>
          <system
                  value="http://terminology.hl7.org/CodeSystem/observation-category"/>
          <code value="vital-signs"/>
          <display value="Vital Signs"/>
        </coding>
      </category>
      <code>
        <coding>
          <system value="http://loinc.org"/>
          <code value="8867-4"/>
          <display value="Heart rate"/>
        </coding>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="147842"/>
          <display value="MDC_ECG_HEART_RATE"/>
        </coding>
      </code>
      <subject>🔗
        <reference value="Patient/SomePatient"/>
      </subject>
      <effectiveDateTime value="2021-07-09T11:33:24+02:00"/>
      <valueQuantity>
        <value value="60"/>
        <unit value="bpm"/>
        <system value="http://unitsofmeasure.org"/>
        <code value="/min"/>
      </valueQuantity>
      <device>🔗
        <reference value="DeviceMetric/HeartRateNumericDeviceMetric"/>
      </device>
    </Observation>