SGHI FHIR Profile Implementation Guide
0.1.0 - ci-build

SGHI FHIR Profile Implementation Guide, published by Kathurima Kimathi. This guide is not an authorized publication; it is the continuous build for version 0.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/savannahghi/sil_fhir_profile_ig/ and changes regularly. See the Directory of published versions

## ValueSet: SGHI Location Form

Official URL: https://fhir.slade360.co.ke/fhir/ValueSet/location-form | Version: 0.1.0
Draft as of 2026-05-21 | Computable Name: SGHILocationForm

Physical form of the location, e.g. building, room, vehicle, road, virtual.

References

- SGHI Location

### Logical Definition (CLD)

- Include these codes as defined in `https://fhir.slade360.co.ke/fhir/CodeSystem/identifier-codesystem` version 📦0.1.0

  Code | Display
  building | Building
  wing | Wing
  ward | Ward
  room | Room
  bed | Bed
  vehicle | Vehicle
  area | Area
  virtual | Virtual

### Expansion

No Expansion for this valueset (Unknown Code System)

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code