@prefix fhir: <http://hl7.org/fhir/> .
@prefix owl: <http://www.w3.org/2002/07/owl#> .
@prefix rdf: <http://www.w3.org/1999/02/22-rdf-syntax-ns#> .
@prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
@prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

# - resource -------------------------------------------------------------------

<http://hl7.org/fhir/CapabilityStatement/messagedefinition> a fhir:CapabilityStatement ;
  fhir:nodeRole fhir:treeRoot ;
  fhir:id [ fhir:v "messagedefinition"] ; # 
  fhir:extension ( [
     fhir:url [
       fhir:v "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg"^^xsd:anyURI ;
       fhir:l <http://hl7.org/fhir/StructureDefinition/structuredefinition-wg>
     ] ;
     fhir:value [
       a fhir:Code ;
       fhir:v "fhir"
     ]
  ] ) ; # 
  fhir:identifier ( [
     fhir:system [
       fhir:v "urn:ietf:rfc:3986"^^xsd:anyURI ;
       fhir:l <urn:ietf:rfc:3986>
     ] ;
     fhir:value [ fhir:v "urn:oid:2.16.840.1.113883.4.642.34.8" ]
  ] ) ; # 
  fhir:status [ fhir:v "draft"] ; # 
  fhir:experimental [ fhir:v true] ; # 
  fhir:date [ fhir:v "2012-01-04"^^xsd:date] ; # 
  fhir:publisher [ fhir:v "HL7 International / FHIR Infrastructure"] ; # 
  fhir:contact ( [
     fhir:telecom ( [
       fhir:system [ fhir:v "url" ] ;
       fhir:value [ fhir:v "http://www.hl7.org/Special/committees/fiwg" ]
     ] )
  ] ) ; # 
  fhir:description [ fhir:v "Sample capability statement showing new MessageDefinition structure"] ; # 
  fhir:kind [ fhir:v "instance"] ; # 
  fhir:software [
     fhir:name [ fhir:v "EHR" ]
  ] ; # 
  fhir:implementation [
     fhir:description [ fhir:v "Acme Message endpoint" ] ;
     fhir:url [
       fhir:v "http://acem.com/fhir/message-drop"^^xsd:anyURI ;
       fhir:l <http://acem.com/fhir/message-drop>
     ]
  ] ; # while the FHIR infrastructure is turning over prior to development, a version is  
#    required.
  fhir:fhirVersion [ fhir:v "6.0.0"] ; # 
  fhir:format ( [ fhir:v "xml"] [ fhir:v "json"] ) ; # this system can do either xml or json. (Listing both implies full support for either, with interconversion)
  fhir:messaging ( [
     fhir:endpoint ( [
       fhir:protocol [
         fhir:system [
           fhir:v "http://hl7.org/fhir/message-transport"^^xsd:anyURI ;
           fhir:l <http://hl7.org/fhir/message-transport>
         ] ;
         fhir:code [ fhir:v "mllp" ]
       ] ;
       fhir:address [
         fhir:v "mllp:10.1.1.10:9234"^^xsd:anyURI ;
         fhir:l fhir:mllp:10.1.1.10:9234
       ] # LLP server at 10.1.1.10 on port 9234
     ] ) ;
     fhir:reliableCache [ fhir:v "30"^^xsd:nonNegativeInteger ] ;
     fhir:documentation [ fhir:v "ADT A08 equivalent for external system notifications" ] ;
     fhir:supportedMessage ( [
       fhir:mode [ fhir:v "receiver" ] ;
       fhir:definition [
         fhir:v "http://hl7.org/fhir/MessageDefinition/example"^^xsd:anyURI ;
         fhir:l <http://hl7.org/fhir/MessageDefinition/example>
       ]
     ] )
  ] ) . # 

# -------------------------------------------------------------------------------------

