US Quality Core Implementation Guide
0.1.0 - cibuild

US Quality Core Implementation Guide, published by ASTP. This guide is not an authorized publication; it is the continuous build for version 0.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/FHIR/us-quality-core/ and changes regularly. See the Directory of published versions

## Resource Profile: USQualityCoreDeviceNotRequested - Detailed Descriptions

Active as of 2019-07-11

Definitions for the us-quality-core-devicenotrequested resource profile.

- Key Elements Table
- Differential Elements Table
- Snapshot Elements Table

Guidance on how to interpret the contents of this table can be foundhere

0. DeviceRequest
Definition | Represents a request for a patient to employ a medical device. The device may be an implantable device, or an external assistive device, such as a walker.
Short | Medical device request
Control | 0..*
Is Modifier | false
Must Support | false
Summary | false
Invariants | dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources (contained.contained.empty()) dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource (contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()) dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated (contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()) dom-5: If a resource is contained in another resource, it SHALL NOT have a security label (contained.meta.security.empty()) dom-6: A resource should have narrative for robust management (text.`div`.exists()) dnr-1: to indicate what device was not requested, either at least one coding in the code or a notDoneValueSet extension shall be provided (`code.extension('http://fhir.org/guides/astp/us-quality-core/StructureDefinition/us-quality-core-notDoneValueSet').exists() xor code.coding.exists()`)
2. DeviceRequest.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Short | A set of rules under which this content was created
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Control | 0..1
Type | uri
Is Modifier | true because This element is labeled as a modifier because the implicit rules may provide additional knowledge about the resource that modifies it's meaning or interpretation
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
4. DeviceRequest.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the resource. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 10..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `DeviceRequest.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
6. DeviceRequest.extension:doNotPerformReason
Slice Name | doNotPerformReason
Definition | Indicates the reason the event was not performed.
Short | Extension
Control | 1..1 This element is affected by the following invariants: ele-1
Type | Extension(US Quality Core Do Not Perform Reason) (Extension Type: CodeableConcept)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
8. DeviceRequest.modifierExtension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the resource and that modifies the understanding of the element that contains it and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer is allowed to define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | ExtensionExtensions that cannot be ignored
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 10..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the resource that contains them
Summary | false
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `DeviceRequest.modifierExtension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
10. DeviceRequest.modifierExtension:doNotPerform
Slice Name | doNotPerform
Definition | An Extension
Short | Extension
Control | 1..1 This element is affected by the following invariants: ele-1
Type | Extension(Extension Definition for DeviceRequest.doNotPerform for Version 5.0) (Extension Type: boolean)
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
12. DeviceRequest.modifierExtension:doNotPerform.extension
Definition | An Extension May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | ExtensionAdditional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..0*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
Slicing | This element introduces a set of slices on `DeviceRequest.modifierExtension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
14. DeviceRequest.modifierExtension:doNotPerform.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/5.0/StructureDefinition/extension-DeviceRequest.doNotPerform`
16. DeviceRequest.modifierExtension:doNotPerform.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 10..1
Type | boolean, date, Meta, Address, Attachment, integer, Count, DataRequirement, Dosage, uuid, Identifier, Coding, SampledData, id, positiveInt, Distance, Period, Duration, canonical, Range, RelatedArtifact, base64Binary, UsageContext, Timing, decimal, CodeableConcept, ParameterDefinition, dateTime, code, string, Contributor, oid, instant, ContactPoint, HumanName, Money, markdown, Ratio, Age, Reference, TriggerDefinition, Quantity, uri, url, Annotation, ContactDetail, Expression, Signature, unsignedInt, time
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Fixed Value | `true`
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
18. DeviceRequest.status
Definition | The status of the request.
Short | draft | active | on-hold | revoked | completed | entered-in-error | unknown
Comments | This element is labeled as a modifier because the status contains the codes cancelled and entered-in-error that mark the request as not currently valid.
Control | 0..1
Binding | The codes SHALL be taken from RequestStatus http://hl7.org/fhir/ValueSet/request-status|4.0.1 (required to `http://hl7.org/fhir/ValueSet/request-status|4.0.1` ) Codes representing the status of the request.
Type | code
Is Modifier | true because This element is labeled as a modifier because it is a status element that contains status entered-in-error which means that the resource should not be treated as valid
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
20. DeviceRequest.intent
Definition | Whether the request is a proposal, plan, an original order or a reflex order.
Short | proposal | plan | directive | order | original-order | reflex-order | filler-order | instance-order | option
Control | 1..1
Binding | The codes SHALL be taken from RequestIntent http://hl7.org/fhir/ValueSet/request-intent|4.0.1 (required to `http://hl7.org/fhir/ValueSet/request-intent|4.0.1` ) The kind of diagnostic request.
Type | code
Is Modifier | true because This element changes the interpretation of all descriptive attributes. For example "the time the request is recommended to occur" vs. "the time the request is authorized to occur" or "who is recommended to perform the request" vs. "who is authorized to perform the request
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
22. DeviceRequest.code[x]
Definition | The details of the device to be used.
Short | (USCDI+ Quality) Device requestedDevice requested
Control | 1..1 This element is affected by the following invariants: dnr-1
Binding | The codes SHOULD be taken from For example codes, see FHIRDeviceTypes http://hl7.org/fhir/ValueSet/device-kind|4.0.1 (preferred to `http://hl7.org/fhir/ValueSet/device-kind` )
Type | CodeableConcept, Reference(Device)
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
24. DeviceRequest.code[x].extension:doNotPerformValueSet
Slice Name | doNotPerformValueSet
Definition | Specifies the value set that characterizes the events or activities that did not occur or were not performed.
Short | What was not done
Control | 0..1 This element is affected by the following invariants: dnr-1
Type | Extension(USQualityCore Not Done ValueSet) (Extension Type: canonical(ValueSet))
Is Modifier | false
Summary | false
Requirements | Must be able to indicate the value set from which the expected event would be drawn, had it occurred.
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count())) ext-1: Must have either extensions or value[x], not both (extension.exists() != value.exists())
26. DeviceRequest.subject
Definition | The patient who will use the device.
Short | Focus of request
Control | 1..1
Type | Reference(US Quality Core Patient, Patient, Group, Location, Device)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))
28. DeviceRequest.authoredOn
Definition | When the request transitioned to being actionable.
Short | When recorded
Control | 10..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (hasValue() or (children().count() > id.count()))

Guidance on how to interpret the contents of this table can be foundhere

0. DeviceRequest
Must Support | false
Invariants | dnr-1: to indicate what device was not requested, either at least one coding in the code or a notDoneValueSet extension shall be provided (`code.extension('http://fhir.org/guides/astp/us-quality-core/StructureDefinition/us-quality-core-notDoneValueSet').exists() xor code.coding.exists()`)
2. DeviceRequest.extension:doNotPerformReason
Slice Name | doNotPerformReason
Short | Extension
Control | 1..1
Type | Extension(US Quality Core Do Not Perform Reason) (Extension Type: CodeableConcept)
4. DeviceRequest.modifierExtension:doNotPerform
Slice Name | doNotPerform
Short | Extension
Control | 1..1
Type | Extension(Extension Definition for DeviceRequest.doNotPerform for Version 5.0) (Extension Type: boolean)
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
6. DeviceRequest.modifierExtension:doNotPerform.value[x]
Short | Value of extension
Control | 1..1
Type | boolean
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Fixed Value | `true`
8. DeviceRequest.status
Short | draft | active | on-hold | revoked | completed | entered-in-error | unknown
10. DeviceRequest.intent
Short | proposal | plan | directive | order | original-order | reflex-order | filler-order | instance-order | option
12. DeviceRequest.code[x]
Short | (USCDI+ Quality) Device requested
Control | 1..1 This element is affected by the following invariants: dnr-1
Binding | The codes SHOULD be taken from FHIRDeviceTypes (preferred to `http://hl7.org/fhir/ValueSet/device-kind` )
Type | CodeableConcept, Reference(Device)
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
14. DeviceRequest.code[x].extension:doNotPerformValueSet
Slice Name | doNotPerformValueSet
Definition | Specifies the value set that characterizes the events or activities that did not occur or were not performed.
Short | What was not done
Control | 0..1 This element is affected by the following invariants: dnr-1
Type | Extension(USQualityCore Not Done ValueSet) (Extension Type: canonical(ValueSet))
Requirements | Must be able to indicate the value set from which the expected event would be drawn, had it occurred.
16. DeviceRequest.subject
Short | Focus of request
Type | Reference(US Quality Core Patient)
18. DeviceRequest.authoredOn
Short | When recorded
Control | 1..1

Guidance on how to interpret the contents of this table can be foundhere

0. DeviceRequest
Definition | Represents a request for a patient to employ a medical device. The device may be an implantable device, or an external assistive device, such as a walker.
Short | Medical device request
Control | 0..*
Is Modifier | false
Must Support | false
Summary | false
Invariants | dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources (`contained.contained.empty()`) dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource (`contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`) dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated (`contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`) dom-5: If a resource is contained in another resource, it SHALL NOT have a security label (`contained.meta.security.empty()`) dom-6: A resource should have narrative for robust management (`text.`div`.exists()`) dnr-1: to indicate what device was not requested, either at least one coding in the code or a notDoneValueSet extension shall be provided (`code.extension('http://fhir.org/guides/astp/us-quality-core/StructureDefinition/us-quality-core-notDoneValueSet').exists() xor code.coding.exists()`)
2. DeviceRequest.id
Definition | The logical id of the resource, as used in the URL for the resource. Once assigned, this value never changes.
Short | Logical id of this artifact
Comments | The only time that a resource does not have an id is when it is being submitted to the server using a create operation.
Control | 0..1
Type | id
Is Modifier | false
Summary | true
4. DeviceRequest.meta
Definition | The metadata about the resource. This is content that is maintained by the infrastructure. Changes to the content might not always be associated with version changes to the resource.
Short | Metadata about the resource
Control | 0..1
Type | Meta
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
6. DeviceRequest.implicitRules
Definition | A reference to a set of rules that were followed when the resource was constructed, and which must be understood when processing the content. Often, this is a reference to an implementation guide that defines the special rules along with other profiles etc.
Short | A set of rules under which this content was created
Comments | Asserting this rule set restricts the content to be only understood by a limited set of trading partners. This inherently limits the usefulness of the data in the long term. However, the existing health eco-system is highly fractured, and not yet ready to define, collect, and exchange data in a generally computable sense. Wherever possible, implementers and/or specification writers should avoid using this element. Often, when used, the URL is a reference to an implementation guide that defines these special rules as part of it's narrative along with other profiles, value sets, etc.
Control | 0..1
Type | uri
Is Modifier | true because This element is labeled as a modifier because the implicit rules may provide additional knowledge about the resource that modifies it's meaning or interpretation
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
8. DeviceRequest.language
Definition | The base language in which the resource is written.
Short | Language of the resource content
Comments | Language is provided to support indexing and accessibility (typically, services such as text to speech use the language tag). The html language tag in the narrative applies to the narrative. The language tag on the resource may be used to specify the language of other presentations generated from the data in the resource. Not all the content has to be in the base language. The Resource.language should not be assumed to apply to the narrative automatically. If a language is specified, it should it also be specified on the div element in the html (see rules in HTML5 for information about the relationship between xml:lang and the html lang attribute).
Control | 0..1
Binding | The codes SHOULD be taken from CommonLanguages (preferred to `http://hl7.org/fhir/ValueSet/languages|4.0.1` ) A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
10. DeviceRequest.text
Definition | A human-readable narrative that contains a summary of the resource and can be used to represent the content of the resource to a human. The narrative need not encode all the structured data, but is required to contain sufficient detail to make it "clinically safe" for a human to just read the narrative. Resource definitions may define what content should be represented in the narrative to ensure clinical safety.
Short | Text summary of the resource, for human interpretation
Comments | Contained resources do not have narrative. Resources that are not contained SHOULD have a narrative. In some cases, a resource may only have text with little or no additional discrete data (as long as all minOccurs=1 elements are satisfied). This may be necessary for data from legacy systems where information is captured as a "text blob" or where text is additionally entered raw or narrated and encoded information is added later.
Control | 0..1
Type | Narrative
Is Modifier | false
Summary | false
Alternate Names | narrative, html, xhtml, display
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
12. DeviceRequest.contained
Definition | These resources do not have an independent existence apart from the resource that contains them - they cannot be identified independently, and nor can they have their own independent transaction scope.
Short | Contained, inline Resources
Comments | This should never be done when the content can be identified properly, as once identification is lost, it is extremely difficult (and context dependent) to restore it again. Contained resources may have profiles and tags In their meta elements, but SHALL NOT have security labels.
Control | 0..*
Type | Resource
Is Modifier | false
Summary | false
Alternate Names | inline resources, anonymous resources, contained resources
14. DeviceRequest.extension
Definition | An Extension
Short | Extension
Control | 1..*
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `DeviceRequest.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
16. DeviceRequest.extension:doNotPerformReason
Slice Name | doNotPerformReason
Definition | Indicates the reason the event was not performed.
Short | Extension
Control | 1..1 This element is affected by the following invariants: ele-1
Type | Extension(US Quality Core Do Not Perform Reason) (Extension Type: CodeableConcept)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
18. DeviceRequest.modifierExtension
Definition | An Extension
Short | Extension
Control | 1..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the resource that contains them
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `DeviceRequest.modifierExtension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
20. DeviceRequest.modifierExtension:doNotPerform
Slice Name | doNotPerform
Definition | An Extension
Short | Extension
Control | 1..1 This element is affected by the following invariants: ele-1
Type | Extension(Extension Definition for DeviceRequest.doNotPerform for Version 5.0) (Extension Type: boolean)
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
22. DeviceRequest.modifierExtension:doNotPerform.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
24. DeviceRequest.modifierExtension:doNotPerform.extension
Definition | An Extension
Short | Extension
Control | 0..0
Type | Extension
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `DeviceRequest.modifierExtension.extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
26. DeviceRequest.modifierExtension:doNotPerform.url
Definition | Source of the definition for the extension code - a logical name or a URL.
Short | identifies the meaning of the extension
Comments | The definition may point directly to a computable or human-readable definition of the extensibility codes, or it may be a logical URI as declared in some other specification. The definition SHALL be a URI for the Structure Definition defining the extension.
Control | 1..1
Type | uri
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
Fixed Value | `http://hl7.org/fhir/5.0/StructureDefinition/extension-DeviceRequest.doNotPerform`
28. DeviceRequest.modifierExtension:doNotPerform.value[x]
Definition | Value of extension - must be one of a constrained set of the data types (see Extensibility for a list).
Short | Value of extension
Control | 1..1
Type | boolean
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Fixed Value | `true`
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
30. DeviceRequest.identifier
Definition | Identifiers assigned to this order by the orderer or by the receiver.
Short | External Request identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 0..*
Type | Identifier
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
32. DeviceRequest.instantiatesCanonical
Definition | The URL pointing to a FHIR-defined protocol, guideline, orderset or other definition that is adhered to in whole or in part by this DeviceRequest.
Short | Instantiates FHIR protocol or definition
Comments | Note: This is a business identifier, not a resource identifier (see discussion). It is best practice for the identifier to only appear on a single resource instance, however business practices may occasionally dictate that multiple resource instances with the same identifier can exist - possibly even with different resource types. For example, multiple Patient and a Person resource instance might share the same social insurance number.
Control | 0..*
Type | canonical(ActivityDefinition, PlanDefinition)
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
34. DeviceRequest.instantiatesUri
Definition | The URL pointing to an externally maintained protocol, guideline, orderset or other definition that is adhered to in whole or in part by this DeviceRequest.
Short | Instantiates external protocol or definition
Comments | This might be an HTML page, PDF, etc. or could just be a non-resolvable URI identifier.
Control | 0..*
Type | uri
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
36. DeviceRequest.basedOn
Definition | Plan/proposal/order fulfilled by this request.
Short | What request fulfills
Control | 0..*
Type | Reference(Resource)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
38. DeviceRequest.priorRequest
Definition | The request takes the place of the referenced completed or terminated request(s).
Short | What request replaces
Control | 0..*
Type | Reference(Resource)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
40. DeviceRequest.groupIdentifier
Definition | Composite request this is part of.
Short | Identifier of composite request
Control | 0..1
Type | Identifier
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
42. DeviceRequest.status
Definition | The status of the request.
Short | draft | active | on-hold | revoked | completed | entered-in-error | unknown
Comments | This element is labeled as a modifier because the status contains the codes cancelled and entered-in-error that mark the request as not currently valid.
Control | 0..1
Binding | The codes SHALL be taken from RequestStatus (required to `http://hl7.org/fhir/ValueSet/request-status|4.0.1` ) Codes representing the status of the request.
Type | code
Is Modifier | true because This element is labeled as a modifier because it is a status element that contains status entered-in-error which means that the resource should not be treated as valid
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
44. DeviceRequest.intent
Definition | Whether the request is a proposal, plan, an original order or a reflex order.
Short | proposal | plan | directive | order | original-order | reflex-order | filler-order | instance-order | option
Control | 1..1
Binding | The codes SHALL be taken from RequestIntent (required to `http://hl7.org/fhir/ValueSet/request-intent|4.0.1` ) The kind of diagnostic request.
Type | code
Is Modifier | true because This element changes the interpretation of all descriptive attributes. For example "the time the request is recommended to occur" vs. "the time the request is authorized to occur" or "who is recommended to perform the request" vs. "who is authorized to perform the request
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
46. DeviceRequest.priority
Definition | Indicates how quickly the {{title}} should be addressed with respect to other requests.
Short | routine | urgent | asap | stat
Control | 0..1
Binding | The codes SHALL be taken from RequestPriority (required to `http://hl7.org/fhir/ValueSet/request-priority|4.0.1` ) Identifies the level of importance to be assigned to actioning the request.
Type | code
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Meaning if Missing | If missing, normal priority
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
48. DeviceRequest.code[x]
Definition | The details of the device to be used.
Short | (USCDI+ Quality) Device requested
Control | 1..1 This element is affected by the following invariants: dnr-1
Binding | The codes SHOULD be taken from FHIRDeviceTypes (preferred to `http://hl7.org/fhir/ValueSet/device-kind` )
Type | CodeableConcept
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
50. DeviceRequest.code[x].id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
52. DeviceRequest.code[x].extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
Slicing | This element introduces a set of slices on `DeviceRequest.code[x].extension`. The slices areUnordered and Open, and can be differentiated using the following discriminators: value @ url
54. DeviceRequest.code[x].extension:doNotPerformValueSet
Slice Name | doNotPerformValueSet
Definition | Specifies the value set that characterizes the events or activities that did not occur or were not performed.
Short | What was not done
Control | 0..1 This element is affected by the following invariants: dnr-1
Type | Extension(USQualityCore Not Done ValueSet) (Extension Type: canonical(ValueSet))
Is Modifier | false
Summary | false
Requirements | Must be able to indicate the value set from which the expected event would be drawn, had it occurred.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
56. DeviceRequest.code[x].coding
Definition | A reference to a code defined by a terminology system.
Short | Code defined by a terminology system
Comments | Codes may be defined very casually in enumerations, or code lists, up to very formal definitions such as SNOMED CT - see the HL7 v3 Core Principles for more information. Ordering of codings is undefined and SHALL NOT be used to infer meaning. Generally, at most only one of the coding values will be labeled as UserSelected = true.
Control | 0..*
Type | Coding
Is Modifier | false
Summary | true
Requirements | Allows for alternative encodings within a code system, and translations to other code systems.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
58. DeviceRequest.code[x].text
Definition | A human language representation of the concept as seen/selected/uttered by the user who entered the data and/or which represents the intended meaning of the user.
Short | Plain text representation of the concept
Comments | Very often the text is the same as a displayName of one of the codings.
Control | 0..1
Type | string
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Requirements | The codes from the terminologies do not always capture the correct meaning with all the nuances of the human using them, or sometimes there is no appropriate code at all. In these cases, the text is used to capture the full meaning of the source.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
60. DeviceRequest.parameter
Definition | Specific parameters for the ordered item. For example, the prism value for lenses.
Short | Device details
Control | 0..*
Type | BackboneElement
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
62. DeviceRequest.parameter.id
Definition | Unique id for the element within a resource (for internal references). This may be any string value that does not contain spaces.
Short | Unique id for inter-element referencing
Control | 0..1
Type | string
Is Modifier | false
XML Format | In the XML format, this property is represented as an attribute.
Summary | false
64. DeviceRequest.parameter.extension
Definition | May be used to represent additional information that is not part of the basic definition of the element. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension.
Short | Additional content defined by implementations
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | false
Summary | false
Alternate Names | extensions, user content
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
66. DeviceRequest.parameter.modifierExtension
Definition | May be used to represent additional information that is not part of the basic definition of the element and that modifies the understanding of the element in which it is contained and/or the understanding of the containing element's descendants. Usually modifier elements provide negation or qualification. To make the use of extensions safe and manageable, there is a strict set of governance applied to the definition and use of extensions. Though any implementer can define an extension, there is a set of requirements that SHALL be met as part of the definition of the extension. Applications processing a resource are required to check for modifier extensions. Modifier extensions SHALL NOT change the meaning of any elements on Resource or DomainResource (including cannot change the meaning of modifierExtension itself).
Short | Extensions that cannot be ignored even if unrecognized
Comments | There can be no stigma associated with the use of extensions by any application, project, or standard - regardless of the institution or jurisdiction that uses or defines the extensions. The use of extensions is what allows the FHIR specification to retain a core level of simplicity for everyone.
Control | 0..*
Type | Extension
Is Modifier | true because Modifier extensions are expected to modify the meaning or interpretation of the element that contains them
Summary | true
Requirements | Modifier extensions allow for extensions that cannot be safely ignored to be clearly distinguished from the vast majority of extensions which can be safely ignored. This promotes interoperability by eliminating the need for implementers to prohibit the presence of extensions. For further information, see the definition of modifier extensions.
Alternate Names | extensions, user content, modifiers
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`) ext-1: Must have either extensions or value[x], not both (`extension.exists() != value.exists()`)
68. DeviceRequest.parameter.code
Definition | A code or string that identifies the device detail being asserted.
Short | Device detail
Control | 0..1
Binding | A code that identifies the device detail.
Type | CodeableConcept
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
70. DeviceRequest.parameter.value[x]
Definition | The value of the device detail.
Short | Value of detail
Comments | Range means device should have a value that falls somewhere within the specified range.
Control | 0..1
Type | Choice of: CodeableConcept, Quantity, Range, boolean
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
72. DeviceRequest.subject
Definition | The patient who will use the device.
Short | Focus of request
Control | 1..1
Type | Reference(US Quality Core Patient)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
74. DeviceRequest.encounter
Definition | An encounter that provides additional context in which this request is made.
Short | Encounter motivating request
Control | 0..1
Type | Reference(Encounter)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
76. DeviceRequest.occurrence[x]
Definition | The timing schedule for the use of the device. The Schedule data type allows many different expressions, for example. "Every 8 hours"; "Three times a day"; "1/2 an hour before breakfast for 10 days from 23-Dec 2011:"; "15 Oct 2013, 17 Oct 2013 and 1 Nov 2013".
Short | Desired time or schedule for use
Control | 0..1
Type | Choice of: dateTime, Period, Timing
[x] Note | SeeChoice of Data Typesfor further information about how to use [x]
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
78. DeviceRequest.authoredOn
Definition | When the request transitioned to being actionable.
Short | When recorded
Control | 1..1
Type | dateTime
Is Modifier | false
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
80. DeviceRequest.requester
Definition | The individual who initiated the request and has responsibility for its activation.
Short | Who/what is requesting diagnostics
Control | 0..1
Type | Reference(Device, Practitioner, PractitionerRole, Organization)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
82. DeviceRequest.performerType
Definition | Desired type of performer for doing the diagnostic testing.
Short | Filler role
Control | 0..1
Binding | For example codes, see ParticipantRoles (example to `http://hl7.org/fhir/ValueSet/participant-role|4.0.1` ) Indicates specific responsibility of an individual within the care team, such as "Primary physician", "Team coordinator", "Caregiver", etc.
Type | CodeableConcept
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
84. DeviceRequest.performer
Definition | The desired performer for doing the diagnostic testing.
Short | Requested Filler
Control | 0..1
Type | Reference(Practitioner, PractitionerRole, Organization, CareTeam, HealthcareService, Patient, Device, RelatedPerson)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
86. DeviceRequest.reasonCode
Definition | Reason or justification for the use of this device.
Short | Coded Reason for request
Control | 0..*
Binding | For example codes, see Condition/Problem/DiagnosisCodes (example to `http://hl7.org/fhir/ValueSet/condition-code|4.0.1` ) Diagnosis or problem codes justifying the reason for requesting the device.
Type | CodeableConcept
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
88. DeviceRequest.reasonReference
Definition | Reason or justification for the use of this device.
Short | Linked Reason for request
Control | 0..*
Type | Reference(Condition, Observation, DiagnosticReport, DocumentReference)
Is Modifier | false
Summary | true
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
90. DeviceRequest.insurance
Definition | Insurance plans, coverage extensions, pre-authorizations and/or pre-determinations that may be required for delivering the requested service.
Short | Associated insurance coverage
Control | 0..*
Type | Reference(Coverage, ClaimResponse)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
92. DeviceRequest.supportingInfo
Definition | Additional clinical information about the patient that may influence the request fulfilment. For example, this may include where on the subject's body the device will be used (i.e. the target site).
Short | Additional clinical information
Control | 0..*
Type | Reference(Resource)
Is Modifier | false
Summary | false
Requirements | Knowing where the device is targeted is important for tracking if multiple sites are possible.
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
94. DeviceRequest.note
Definition | Details about this request that were not represented at all or sufficiently in one of the attributes provided in a class. These may include for example a comment, an instruction, or a note associated with the statement.
Short | Notes or comments
Control | 0..*
Type | Annotation
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)
96. DeviceRequest.relevantHistory
Definition | Key events in the history of the request.
Short | Request provenance
Comments | This might not include provenances for all versions of the request - only those deemed "relevant" or important. This SHALL NOT include the Provenance associated with this current version of the resource. (If that provenance is deemed to be a "relevant" change, it will need to be added as part of a later update. Until then, it can be queried directly as the Provenance that points to this version using _revinclude All Provenances should have some historical version of this Request as their subject.
Control | 0..*
Type | Reference(Provenance)
Is Modifier | false
Summary | false
Invariants | ele-1: All FHIR elements must have a @value or children (`hasValue() or (children().count() > id.count())`)