HL7 Czech Imaging Order IG
0.1.0-ballot - ballot

HL7 Czech Imaging Order IG, published by HL7 Czech Republic. This guide is not an authorized publication; it is the continuous build for version 0.1.0-ballot built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7-cz/img-order/ and changes regularly. See the Directory of published versions

## : MRDevice - XML Representation

Raw xml | Download

    <Device xmlns="http://hl7.org/fhir">
      <id value="MRDevice"/>
      <meta>
        <profile
                 value="https://hl7.cz/fhir/core/StructureDefinition/cz-device-observer"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: Device MRDevice</b></p><a name="MRDevice"> </a><a name="hcMRDevice"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="https://build.fhir.org/ig/HL7-cz/cz-core/StructureDefinition-cz-device-observer.html">Device: Performer/Observer (CZ)</a></p></div><p><b>type</b>: <span title="Codes:{http://snomed.info/sct 90003000}">Magnetic resonance imaging unit</span></p></div>
      </text>
      <type>
        <coding>
          <system value="http://snomed.info/sct"/>
          <code value="90003000"/>
          <display value="Magnetic resonance imaging unit"/>
        </coding>
      </type>
    </Device>