HL7 Czech Imaging Order IG
0.1.0-ballot - ballot

HL7 Czech Imaging Order IG, published by HL7 Czech Republic. This guide is not an authorized publication; it is the continuous build for version 0.1.0-ballot built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7-cz/img-order/ and changes regularly. See the Directory of published versions

## ValueSet: ObservationsUnitHeight

Official URL: https://ncez.mzcr.cz/terminology/ValueSet/observationUnitsHeight-cz | Version: 0.1.0-ballot
Standards status: Trial-use | Maturity Level: 2 | Computable Name: CZ_ObservationUnitsHeightVs

UCUM units for height

References

- Body Height: Imaging Order (CZ)

### Logical Definition (CLD)

Language: cs

- Include these codes as defined in `http://unitsofmeasure.org` version Not Stated (use latest from terminology server)

  Code | Display
  m |
  cm |

### Expansion

Expansion from tx.fhir.org based on codesystem UCUM version 2.2

This value set contains 2 concepts

System | Code | Display (cs) - Czech (cs) | JSON | XML
`http://unitsofmeasure.org` | m |  |  |
`http://unitsofmeasure.org` | cm |  |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code