HL7 Czech Imaging Order IG
0.1.0-ballot - ballot

HL7 Czech Imaging Order IG, published by HL7 Czech Republic. This guide is not an authorized publication; it is the continuous build for version 0.1.0-ballot built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7-cz/img-order/ and changes regularly. See the Directory of published versions

## ValueSet: CZ Modality

Official URL: https://ncez.mzcr.cz/terminology/ValueSet/cz-modality | Version: 0.1.0-ballot
Active as of 2019-03-27 | Computable Name: CZ_ModalityVs

This value set includes all modalities.

References

- Service Request: Imaging Order (CZ)

### Logical Definition (CLD)

Language: cs

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM` version 📍2022.4.20221006

  Code | Display | Definition
  `AR` | Autorefraction | An acquisition device, process or method that measures autorefraction.
  `BI` | Biomagnetic Imaging | An acquisition device, process or method that performs biomagnetic imaging.
  `BMD` | Bone Mineral Densitometry | An acquisition device, process or method that performs bone mineral densitometry by X-Ray, including dual-energy X-Ray absorptiometry (DXA) and morphometric X-Ray absorptiometry (MXA).
  `CR` | Computed Radiography | An acquisition device, process or method that performs computed radiography.
  `CT` | Computed Tomography | An acquisition device, process or method that performs computed tomography.
  `DMS` | Dermoscopy | An acquisition device, process or method that performs imaging of the surface of the skin using epiluminescence microscopy.
  `DG` | Diaphanography | An acquisition device, process or method that performs diaphanography.
  `DX` | Digital Radiography | An acquisition device, process or method that performs digital radiography.
  `ES` | Endoscopy | An acquisition device, process or method that records images during endoscopy.
  `XC` | External-camera Photography | An acquisition device, process or method that performs photography with an external camera.
  `GM` | General Microscopy | An acquisition device, process or method that performs general microscopy.
  `IO` | Intra-oral Radiography | An acquisition device, process or method that performs intra-oral radiography.
  `IVOCT` | Intravascular Optical Coherence Tomography | An acquisition device, process or method that performs intravascular optical coherence tomography
  `IVUS` | Intravascular Ultrasound | An acquisition device, process or method that performs intravascular ultrasound.
  `KER` | Keratometry | An acquisition device, process or method that performs keratometry.
  `LS` | Laser surface scan | An acquisition device, process or method that performs laser surface scanning.
  `LEN` | Lensometry | An acquisition device, process or method that performs lensometry.
  `MR` | Magnetic Resonance | An acquisition device, process or method that performs magnetic resonance imaging.
  `MG` | Mammography | An acquisition device, process or method that performs mammography.
  `NM` | Nuclear Medicine | An acquisition device, process or method that performs nuclear medicine imaging.
  `OAM` | Ophthalmic Axial Measurements | An acquisition device, process or method that measures the axial length of the eye.
  `OPM` | Ophthalmic Mapping | An acquisition device, process or method that measures corneal topography, corneal or retinal thickness, and other similar parameters that are typically displayed as maps.
  `OP` | Ophthalmic Photography | An acquisition device, process or method that performs ophthalmic photography.
  `OPT` | Ophthalmic Tomography | An acquisition device, process or method that performs tomography of the eye that is based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
  `OPTBSV` | Ophthalmic Tomography B-scan Volume Analysis | An acquisition device, process or method that performs B-scan volume analysis of tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
  `OPTENF` | Ophthalmic Tomography En Face | An acquisition device, process or method that creates en face tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
  `OPV` | Ophthalmic Visual Field | An acquisition device, process or method that measures visual fields and perform visual perimetry.
  `OCT` | Optical Coherence Tomography | An acquisition device, process or method that uses an interferometric, non-invasive optical tomographic technique to image 2D slices and 3D volumes of tissue using visible and near visible frequencies.
  `OSS` | Optical Surface Scanner | An acquisition device, process or method that performs optical surface scanning.
  `PX` | Panoramic X-Ray | An acquisition device, process or method that performs panoramic X-Rays.
  `PT` | Positron emission tomography | An acquisition device, process or method that performs positron emission tomography (PET).
  `RF` | Radiofluoroscopy | An acquisition device, process or method that performs radiofluoroscopy.
  `RG` | Radiographic imaging | An acquisition device, process or method that performs radiographic imaging (conventional film/screen).
  `RTIMAGE` | RT Image | An acquisition device, process or method that performs radiotherapy imaging; includes portal imaging.
  `SM` | Slide Microscopy | An acquisition device, process or method that performs slide microscopy.
  `SRF` | Subjective Refraction | An acquisition device, process or method that records subjective refraction.
  `TG` | Thermography | An acquisition device, process or method that performs thermography.
  `US` | Ultrasound | An acquisition device, process or method that performs ultrasound.
  `BDUS` | Ultrasound Bone Densitometry | An acquisition device, process or method that performs ultrasound bone densitometry.
  `VA` | Visual Acuity | An acquisition device, process or method that measures visual acuity.
  `XA` | X-Ray Angiography | An acquisition device, process or method that performs X-Ray angiography.

### Expansion

Expansion performed internally based on codesystem DICOM v2022.4.20221006 (CodeSystem)

This value set contains 41 concepts

System | Code | Display (cs) | Definition | JSON | XML
`http://dicom.nema.org/resources/ontology/DCM` | `AR` | Autorefraction | An acquisition device, process or method that measures autorefraction. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `BI` | Biomagnetic Imaging | An acquisition device, process or method that performs biomagnetic imaging. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `BMD` | Bone Mineral Densitometry | An acquisition device, process or method that performs bone mineral densitometry by X-Ray, including dual-energy X-Ray absorptiometry (DXA) and morphometric X-Ray absorptiometry (MXA). |  |
`http://dicom.nema.org/resources/ontology/DCM` | `CR` | Computed Radiography | An acquisition device, process or method that performs computed radiography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `CT` | Computed Tomography | An acquisition device, process or method that performs computed tomography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `DMS` | Dermoscopy | An acquisition device, process or method that performs imaging of the surface of the skin using epiluminescence microscopy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `DG` | Diaphanography | An acquisition device, process or method that performs diaphanography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `DX` | Digital Radiography | An acquisition device, process or method that performs digital radiography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `ES` | Endoscopy | An acquisition device, process or method that records images during endoscopy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `XC` | External-camera Photography | An acquisition device, process or method that performs photography with an external camera. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `GM` | General Microscopy | An acquisition device, process or method that performs general microscopy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `IO` | Intra-oral Radiography | An acquisition device, process or method that performs intra-oral radiography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `IVOCT` | Intravascular Optical Coherence Tomography | An acquisition device, process or method that performs intravascular optical coherence tomography |  |
`http://dicom.nema.org/resources/ontology/DCM` | `IVUS` | Intravascular Ultrasound | An acquisition device, process or method that performs intravascular ultrasound. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `KER` | Keratometry | An acquisition device, process or method that performs keratometry. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `LS` | Laser surface scan | An acquisition device, process or method that performs laser surface scanning. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `LEN` | Lensometry | An acquisition device, process or method that performs lensometry. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `MR` | Magnetic Resonance | An acquisition device, process or method that performs magnetic resonance imaging. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `MG` | Mammography | An acquisition device, process or method that performs mammography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `NM` | Nuclear Medicine | An acquisition device, process or method that performs nuclear medicine imaging. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OAM` | Ophthalmic Axial Measurements | An acquisition device, process or method that measures the axial length of the eye. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OPM` | Ophthalmic Mapping | An acquisition device, process or method that measures corneal topography, corneal or retinal thickness, and other similar parameters that are typically displayed as maps. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OP` | Ophthalmic Photography | An acquisition device, process or method that performs ophthalmic photography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OPT` | Ophthalmic Tomography | An acquisition device, process or method that performs tomography of the eye that is based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OPTBSV` | Ophthalmic Tomography B-scan Volume Analysis | An acquisition device, process or method that performs B-scan volume analysis of tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OPTENF` | Ophthalmic Tomography En Face | An acquisition device, process or method that creates en face tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OPV` | Ophthalmic Visual Field | An acquisition device, process or method that measures visual fields and perform visual perimetry. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OCT` | Optical Coherence Tomography | An acquisition device, process or method that uses an interferometric, non-invasive optical tomographic technique to image 2D slices and 3D volumes of tissue using visible and near visible frequencies. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `OSS` | Optical Surface Scanner | An acquisition device, process or method that performs optical surface scanning. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `PX` | Panoramic X-Ray | An acquisition device, process or method that performs panoramic X-Rays. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `PT` | Positron emission tomography | An acquisition device, process or method that performs positron emission tomography (PET). |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RF` | Radiofluoroscopy | An acquisition device, process or method that performs radiofluoroscopy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RG` | Radiographic imaging | An acquisition device, process or method that performs radiographic imaging (conventional film/screen). |  |
`http://dicom.nema.org/resources/ontology/DCM` | `RTIMAGE` | RT Image | An acquisition device, process or method that performs radiotherapy imaging; includes portal imaging. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `SM` | Slide Microscopy | An acquisition device, process or method that performs slide microscopy. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `SRF` | Subjective Refraction | An acquisition device, process or method that records subjective refraction. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `TG` | Thermography | An acquisition device, process or method that performs thermography. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `US` | Ultrasound | An acquisition device, process or method that performs ultrasound. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `BDUS` | Ultrasound Bone Densitometry | An acquisition device, process or method that performs ultrasound bone densitometry. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `VA` | Visual Acuity | An acquisition device, process or method that measures visual acuity. |  |
`http://dicom.nema.org/resources/ontology/DCM` | `XA` | X-Ray Angiography | An acquisition device, process or method that performs X-Ray angiography. |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code