HL7 Czech Imaging Order IG
0.1.0-ballot - ballot

HL7 Czech Imaging Order IG, published by HL7 Czech Republic. This guide is not an authorized publication; it is the continuous build for version 0.1.0-ballot built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7-cz/img-order/ and changes regularly. See the Directory of published versions

## ValueSet: CZ Mobility Value

Official URL: https://ncez.mzcr.cz/terminology/ValueSet/cz-mobility-value | Version: 0.1.0-ballot
Active as of 2026-01-01 | Computable Name: CZ_MobilityValueVs
Copyright/Legal: This value set includes content from SNOMED CT, which is copyright © 2002+ International Health Terminology Standards Development Organisation (IHTSDO), and distributed by agreement between IHTSDO and HL7. Implementer use of SNOMED CT is not covered by this agreement

This value set includes all patient im/mobility values for imaging order.

References

- Patient mobility: Imaging Order (CZ)

### Logical Definition (CLD)

Language: cs

- Include these codes as defined in `http://snomed.info/sct` version Not Stated (use latest from terminology server)

  Code | Display
  282146009 | Does walk
  282147000 | Does not walk
  282873007 | Does stand up
  282874001 | Does not stand up
  282972001 | Does stand
  282973006 | Does not stand
  301683006 | Does move in bed
  301684000 | Does not move in bed

### Expansion

Expansion from tx.hl7europe.eu based on SNOMED CT 11000279109 edition 27-Jan 2025

This value set contains 8 concepts

System | Code | Display (cs) - Czech (cs) | JSON | XML
`http://snomed.info/sct` | 282146009 |  |  |
`http://snomed.info/sct` | 282147000 |  |  |
`http://snomed.info/sct` | 282873007 |  |  |
`http://snomed.info/sct` | 282874001 |  |  |
`http://snomed.info/sct` | 282972001 |  |  |
`http://snomed.info/sct` | 282973006 |  |  |
`http://snomed.info/sct` | 301683006 |  |  |
`http://snomed.info/sct` | 301684000 |  |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code