US Core Implementation Guide
8.0.1 - STU 8

US Core Implementation Guide, published by HL7 International / Cross-Group Projects. This guide is not an authorized publication; it is the continuous build for version 8.0.1 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/US-Core/ and changes regularly. See the Directory of published versions

## SearchParameter: USCoreDeviceType

Official URL: http://hl7.org/fhir/us/core/SearchParameter/us-core-device-type | Version: 8.0.1
Standards status: Trial-use | Maturity Level: 3 | Computable Name: USCoreDeviceType
Other Identifiers: OID:2.16.840.1.113883.4.642.40.2.40.23
Copyright/Legal: Used by permission of HL7 International, all rights reserved Creative Commons License

The type of the device
NOTE: This SearchParameter is defined only to document Server and Client expectations. Its definition is derived from the standard FHIR SearchParameter and it uses the Conformance expectation extension to define additional expectations for the following SearchParameter elements:

- `multipleAnd`
- `multipleOr`
- `comparator`
- `modifier`
- `chain`

It SHALL NOT be used as a search parameter for search. Servers and Clients SHOULD use the standard FHIR SearchParameter.

id us-core-device-type

url : http://hl7.org/fhir/us/core/SearchParameter/us-core-device-type

name : USCoreDeviceType

derivedFrom : http://hl7.org/fhir/SearchParameter/Device-type

status : active

date : 11/17/2024

publisher : HL7 International - Cross-Group Projects

contact : http://www.hl7.org/Special/committees/cgp

jurisdiction : United States of America (the) (Details : {urn:iso:std:iso:3166 code 'US' = 'United States of America', given as 'United States of America (the)'})

code : `type`

base :Device

type : token

expression : `Device.type`

xpath : `f:Device/f:type`

xpathUsage : normal

multipleOr : True (Conformance Expectation = MAY)

multipleAnd : True ( Conformance Expectation = MAY)