Vital Signs with Qualifying Elements
2.0.0 - ci-build

Vital Signs with Qualifying Elements, published by HL7 International - Clinical Information Modeling Initiative. This guide is not an authorized publication; it is the continuous build for version 2.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/cimi-vital-signs/ and changes regularly. See the Directory of published versions

## ValueSet: Weight Measurement Device value set

Official URL: http://hl7.org/fhir/us/vitals/ValueSet/weightMeasurementDeviceVS | Version: 2.0.0
Draft as of 2024-10-09 | Computable Name: WeightMeasurementDevice
Copyright/Legal: This value set includes content from SNOMED CT, which is copyright © 2002+ International Health Terminology Standards Development Organisation (IHTSDO), and distributed by agreement between IHTSDO and HL7. Implementer use of SNOMED CT is not covered by this agreement

SELECT SNOMED CT code system values that descibe the instrument used to measure the body weight.

References

- Body Weight

### Logical Definition (CLD)

Generated Narrative: ValueSet weightMeasurementDeviceVS

This value set includes codes based on the following rules:

- Include these codes as defined in `http://snomed.info/sct`

  Code | Display
  466289007 | Bed scale (physical object)
  444063009 | Broselow Luten color coding system for pediatric weight estimation (assessment scale)
  720689000 | Chair scale (physical object)
  469204003 | Floor scale, electronic (physical object)
  469787007 | Floor scale, mechanical (physical object)
  58514003 | Infant scale (physical object)
  462242008 | Patient sling scale (physical object)
  466532009 | Wheelchair scale (physical object)

- Include these codes as defined in `http://hl7.org/fhir/us/vitals/CodeSystem/SolorTemporaryCodeSystem`

  Code | Display | Definition
  24181000205106 | Patient lift scale (physical object) | A device used to lift a patient out of or into bed and also has a scale to measure the subject's weight.

### Expansion

Generated Narrative: ValueSet

Expansion based on:

- codesystem SNOMED CT Solor Extension Temporary Code System v2.0.0 (CodeSystem)
- SNOMED CT United States edition 01-Mar 2024

This value set contains 9 concepts

Code | System | Display | Definition
466289007 | http://snomed.info/sct | Bed scale (physical object) |
444063009 | http://snomed.info/sct | Broselow Luten color coding system for pediatric weight estimation (assessment scale) |
720689000 | http://snomed.info/sct | Chair scale (physical object) |
469204003 | http://snomed.info/sct | Floor scale, electronic (physical object) |
469787007 | http://snomed.info/sct | Floor scale, mechanical |
58514003 | http://snomed.info/sct | Infant scale |
462242008 | http://snomed.info/sct | Patient sling scale |
466532009 | http://snomed.info/sct | Wheelchair scale (physical object) |
24181000205106 | http://hl7.org/fhir/us/vitals/CodeSystem/SolorTemporaryCodeSystem | Patient lift scale (physical object) | A device used to lift a patient out of or into bed and also has a scale to measure the subject's weight.

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code