## Intersection of http://hl7.org/fhir/us/vitals/StructureDefinition/bp-device and http://hl7.org/fhir/us/vitals/StructureDefinition/bp-device

This is the set of resources that conform to both Blood Pressure Device (http://hl7.org/fhir/us/vitals/StructureDefinition/bp-device) and Blood Pressure Device (http://hl7.org/fhir/us/vitals/StructureDefinition/bp-device).

### Structure

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* |  | Item used in healthcare dom-2: If the resource is contained in another resource, it SHALL NOT contain nested Resources dom-3: If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource dom-4: If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated dom-5: If a resource is contained in another resource, it SHALL NOT have a security label dom-6: A resource should have narrative for robust management
meta | Σ | 0..1 | Meta | Metadata about the resource ele-1: All FHIR elements must have a @value or children
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created ele-1: All FHIR elements must have a @value or children
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
ele-1: All FHIR elements must have a @value or children
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation ele-1: All FHIR elements must have a @value or children
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Extension ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
identifier |  | 0..* | Identifier | Instance identifier ele-1: All FHIR elements must have a @value or children
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device ele-1: All FHIR elements must have a @value or children
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI ele-1: All FHIR elements must have a @value or children
issuer |  | 0..1 | uri | UDI Issuing Organization ele-1: All FHIR elements must have a @value or children
jurisdiction |  | 0..1 | uri | Regional UDI authority ele-1: All FHIR elements must have a @value or children
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String ele-1: All FHIR elements must have a @value or children
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String ele-1: All FHIR elements must have a @value or children
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. ele-1: All FHIR elements must have a @value or children
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. ele-1: All FHIR elements must have a @value or children
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. ele-1: All FHIR elements must have a @value or children
distinctIdentifier |  | 0..1 | string | The distinct identification string ele-1: All FHIR elements must have a @value or children
manufacturer |  | 0..1 | string | Name of device manufacturer ele-1: All FHIR elements must have a @value or children
manufactureDate |  | 0..1 | dateTime | Date when the device was made ele-1: All FHIR elements must have a @value or children
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) ele-1: All FHIR elements must have a @value or children
lotNumber |  | 0..1 | string | Lot number of manufacture ele-1: All FHIR elements must have a @value or children
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer ele-1: All FHIR elements must have a @value or children
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
name |  | 1..1 | string | The name of the device ele-1: All FHIR elements must have a @value or children
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. ele-1: All FHIR elements must have a @value or children
modelNumber |  | 0..1 | string | The model number for the device ele-1: All FHIR elements must have a @value or children
partNumber |  | 0..1 | string | The part number of the device ele-1: All FHIR elements must have a @value or children
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: ?? (extensible) ele-1: All FHIR elements must have a @value or children
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate ele-1: All FHIR elements must have a @value or children
version |  | 0..1 | string | The version of the standard that is used to operate and communicate ele-1: All FHIR elements must have a @value or children
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
type |  | 0..1 | CodeableConcept | The type of the device version ele-1: All FHIR elements must have a @value or children
component |  | 0..1 | Identifier | A single component of the device version ele-1: All FHIR elements must have a @value or children
value |  | 1..1 | string | The version text ele-1: All FHIR elements must have a @value or children
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties ele-1: All FHIR elements must have a @value or children
extension |  | 0..* | Extension | Additional content defined by implementations ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized ele-1: All FHIR elements must have a @value or children ext-1: Must have either extensions or value[x], not both
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) ele-1: All FHIR elements must have a @value or children
valueQuantity |  | 0..* | Quantity | Property value as a quantity ele-1: All FHIR elements must have a @value or children
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) ele-1: All FHIR elements must have a @value or children
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed ele-1: All FHIR elements must have a @value or children
owner |  | 0..1 | Reference(Organization) | Organization responsible for device ele-1: All FHIR elements must have a @value or children
contact |  | 0..* | ContactPoint | Details for human/organization for support ele-1: All FHIR elements must have a @value or children
location |  | 0..1 | Reference(Location) | Where the device is found ele-1: All FHIR elements must have a @value or children
url |  | 0..1 | uri | Network address to contact device ele-1: All FHIR elements must have a @value or children
note |  | 0..* | Annotation | Device notes and comments ele-1: All FHIR elements must have a @value or children
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device ele-1: All FHIR elements must have a @value or children
parent |  | 0..1 | Reference(Device) | The parent device ele-1: All FHIR elements must have a @value or children
Documentation for this format