Vital Signs with Qualifying Elements
2.0.0 - ci-build

Vital Signs with Qualifying Elements, published by HL7 International - Clinical Information Modeling Initiative. This guide is not an authorized publication; it is the continuous build for version 2.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/cimi-vital-signs/ and changes regularly. See the Directory of published versions

## Resource Profile: Blood Pressure Device

Official URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-device | Version: 2.0.0
Draft as of 2024-10-09 | Computable Name: BloodPressureDevice
Copyright/Legal: Logica Health, all rights reserved Creative Commons License

A profile of the Device resource used specifically for blood pressure devices and includes an extension for blood pressure cuff size.

### Blood Pressure Device profile

This profile is used specifically for blood pressure measurements. It incorporates an extension for blood pressure device cuff size.

#### Examples

The following examples are provided to illustrate conformant resource content to this profile.

Blood Pressure Device Example 1

Blood Pressure Device Example 2

Usage:

- Refer to this Resource Profile: Average Blood Pressure, Blood Pressure Panel and Twenty Four Hour Blood Pressure
- Examples for this Resource Profile: Device/BPDevice1-example and Device/BPDevice2-example

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Differential Table
- Key Elements Table
- Snapshot Table
- Statistics/References
- All

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  |  | Device |
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
Documentation for this format

#### Terminology Bindings (Differential)

Path | Conformance | ValueSet | URI
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Device.status | required | FHIRDeviceStatus `http://hl7.org/fhir/ValueSet/device-status|4.0.1` from the FHIR Standard
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Device.language | preferred | CommonLanguages
Additional Bindings | Purpose
AllLanguages | Max Binding
`http://hl7.org/fhir/ValueSet/languages` from the FHIR Standard
Device.udiCarrier.entryType | required | UDIEntryType `http://hl7.org/fhir/ValueSet/udi-entry-type|4.0.1` from the FHIR Standard
Device.status | required | FHIRDeviceStatus `http://hl7.org/fhir/ValueSet/device-status|4.0.1` from the FHIR Standard
Device.statusReason | extensible | FHIRDeviceStatusReason `http://hl7.org/fhir/ValueSet/device-status-reason` from the FHIR Standard
Device.deviceName.type | required | DeviceNameType `http://hl7.org/fhir/ValueSet/device-nametype|4.0.1` from the FHIR Standard
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

This structure is derived from Device

Summary

Extensions

This structure refers to these extensions:

- http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext

Differential View

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  |  | Device |
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
Documentation for this format

#### Terminology Bindings (Differential)

Path | Conformance | ValueSet | URI
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

Key Elements View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Device.status | required | FHIRDeviceStatus `http://hl7.org/fhir/ValueSet/device-status|4.0.1` from the FHIR Standard
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

Snapshot View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
Slices for extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
cuffSize |  | 0..* | CodeableConcept | Cuff Size URL: http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext Binding: Blood Pressure Cuff Size value set (extensible)
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: Blood Pressure Measurement Device value set (extensible)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Conformance | ValueSet | URI
Device.language | preferred | CommonLanguages
Additional Bindings | Purpose
AllLanguages | Max Binding
`http://hl7.org/fhir/ValueSet/languages` from the FHIR Standard
Device.udiCarrier.entryType | required | UDIEntryType `http://hl7.org/fhir/ValueSet/udi-entry-type|4.0.1` from the FHIR Standard
Device.status | required | FHIRDeviceStatus `http://hl7.org/fhir/ValueSet/device-status|4.0.1` from the FHIR Standard
Device.statusReason | extensible | FHIRDeviceStatusReason `http://hl7.org/fhir/ValueSet/device-status-reason` from the FHIR Standard
Device.deviceName.type | required | DeviceNameType `http://hl7.org/fhir/ValueSet/device-nametype|4.0.1` from the FHIR Standard
Device.type | extensible | BloodPressureMeasurementDevicevalueset `http://hl7.org/fhir/us/vitals/ValueSet/bpMeasDeviceVS` from this IG

This structure is derived from Device

Summary

Extensions

This structure refers to these extensions:

- http://hl7.org/fhir/us/vitals/StructureDefinition/bp-cuff-size-ext

Other representations of profile: CSV, Excel, Schematron