## Profile Comparison between http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips vs http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips

Left: | Device - performer, observer (http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips)
Right: | Device - Performer or Observer (IPS) (http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips)

### Messages

Error | StructureDefinition.version | Values for version differ: '2.0.0-ballot' vs '2.0.0'
Information | StructureDefinition.title | Values for title differ: 'Device - performer, observer' vs 'Device - Performer or Observer (IPS)'
Information | StructureDefinition.comment | Values for comment differ: 'UDI may identify an unique instance of a device, or it may only identify the type of the device. See [UDI mappings](device-mappings.html#udi) for a complete mapping of UDI parts to Device.' vs 'UDI may identify an unique instance of a device, or it may only identify the type of the device. See [UDI mappings](http://hl7.org/fhir/R4/device-mappings.html#udi) for a complete mapping of UDI parts to Device.'

### Metadata

Name | Value | Comments
--- | --- | ---
abstract | false |
baseDefinition | http://hl7.org/fhir/StructureDefinition/Device |
copyright |  |
date | 2024-06-19T10:50:07-05:00 |
description | This profile represents the constraints applied to the Device resource by the IPS project, which specifies an international patient summary based on the FHIR standard R4.; This profile describes a device that plays the role of observer or performer. | This profile represents the constraints applied to the Device resource by the IPS project, which specifies an international patient summary based on the FHIR standard R4. This profile describes a device that plays the role of observer or performer. | Values Differ
experimental |  |
fhirVersion | 4.0.1 |
jurisdiction |  |
jurisdiction[0] | http://unstats.un.org/unsd/methods/m49/m49.htm#001 |
kind | resource |
name | DeviceObserverUvIps |
publisher | HL7 International / Patient Care |
purpose | This profile constrains the representation of a device acting as observer in the international patient summary as specified by the IPS project. |
status | active |
title | Device - performer, observer | Device - Performer or Observer (IPS) | Values Differ
type | Device |
url | http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips |
version | 2.0.0-ballot | 2.0.0 | Values Differ

### Structure

Name | L Flags | L Card. | L Type | L Description & Constraints | R Flags | R Card. | R Type | R Description & Constraints | Comments
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare |  | 0..* | Device | Item used in healthcare |
id | Σ | 0..1 | id | Logical id of this artifact | Σ | 0..1 | id | Logical id of this artifact |
meta | Σ | 0..1 | Meta | Metadata about the resource | Σ | 0..1 | Meta | Metadata about the resource |
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created | ?!Σ | 0..1 | uri | A set of rules under which this content was created |
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
|  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements |
contained |  | 0..* | Resource | Contained, inline Resources |  | 0..* | Resource | Contained, inline Resources |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored | ?! | 0..* | Extension | Extensions that cannot be ignored |
identifier | S | 0..* | Identifier | Instance identifier | SO | 0..* | Identifier | Instance identifier
Obligations | Actor
SHALL:populate-if-known | Creator (IPS)
SHALL:handle | Consumer (IPS)
SHOULD:display | Consumer (IPS)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device |
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI | Σ | 0..1 | string | Mandatory fixed portion of UDI |
issuer |  | 0..1 | uri | UDI Issuing Organization |  | 0..1 | uri | UDI Issuing Organization |
jurisdiction |  | 0..1 | uri | Regional UDI authority |  | 0..1 | uri | Regional UDI authority |
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String |
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String | Σ | 0..1 | string | UDI Human Readable Barcode String |
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered. |
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device. |
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device. |
distinctIdentifier |  | 0..1 | string | The distinct identification string |  | 0..1 | string | The distinct identification string |
manufacturer | S | 0..1 | string | Name of device manufacturer | SO | 0..1 | string | Name of device manufacturer
Obligations | Actor
SHALL:populate-if-known | Creator (IPS)
SHALL:handle | Consumer (IPS)
SHOULD:display | Consumer (IPS)
manufactureDate |  | 0..1 | dateTime | Date when the device was made |  | 0..1 | dateTime | Date when the device was made |
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable) |
lotNumber |  | 0..1 | string | Lot number of manufacture |  | 0..1 | string | Lot number of manufacture |
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer |  | 0..1 | string | Serial number assigned by the manufacturer |
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer |  | 0..* | BackboneElement | The name of the device as given by the manufacturer |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
name |  | 1..1 | string | The name of the device |  | 1..1 | string | The name of the device |
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by. |
modelNumber | S | 0..1 | string | The model number for the device | SO | 0..1 | string | The model number for the device
Obligations | Actor
SHALL:populate-if-known | Creator (IPS)
SHALL:handle | Consumer (IPS)
SHOULD:display | Consumer (IPS)
partNumber |  | 0..1 | string | The part number of the device |  | 0..1 | string | The part number of the device |
type |  | 0..1 | CodeableConcept | The kind or type of device Binding: ?? (example): Codes to identify medical devices. |  | 0..1 | CodeableConcept | The kind or type of device Binding: ?? (example): Codes to identify medical devices. |
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate |
version |  | 0..1 | string | The version of the standard that is used to operate and communicate |  | 0..1 | string | The version of the standard that is used to operate and communicate |
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device |  | 0..* | BackboneElement | The actual design of the device or software version running on the device |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 0..1 | CodeableConcept | The type of the device version |  | 0..1 | CodeableConcept | The type of the device version |
component |  | 0..1 | Identifier | A single component of the device version |  | 0..1 | Identifier | A single component of the device version |
value |  | 1..1 | string | The version text |  | 1..1 | string | The version text |
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties |
id |  | 0..1 | string | Unique id for inter-element referencing |  | 0..1 | string | Unique id for inter-element referencing |
extension |  | 0..* | Extension | Additional content defined by implementations |  | 0..* | Extension | Additional content defined by implementations |
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized |
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible) |
valueQuantity |  | 0..* | Quantity | Property value as a quantity |  | 0..* | Quantity | Property value as a quantity |
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP) |
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed |
owner |  | 0..1 | Reference(Organization) | Organization responsible for device |  | 0..1 | Reference(Organization) | Organization responsible for device |
contact |  | 0..* | ContactPoint | Details for human/organization for support |  | 0..* | ContactPoint | Details for human/organization for support |
location |  | 0..1 | Reference(Location) | Where the device is found |  | 0..1 | Reference(Location) | Where the device is found |
url |  | 0..1 | uri | Network address to contact device |  | 0..1 | uri | Network address to contact device |
note |  | 0..* | Annotation | Device notes and comments |  | 0..* | Annotation | Device notes and comments |
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device | Σ | 0..* | CodeableConcept | Safety Characteristics of Device |
parent |  | 0..1 | Reference(Device) | The parent device |  | 0..1 | Reference(Device) | The parent device |
Documentation for this format