Moderne Patient:innenabrechnung und Datenkommunikation on FHIR (MOPED)
0.1.0 - ci-build

Moderne Patient:innenabrechnung und Datenkommunikation on FHIR (MOPED), published by ELGA GmbH. This guide is not an authorized publication; it is the continuous build for version 0.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7Austria/ELGA-MOPED-R5/ and changes regularly. See the Directory of published versions

## Resource Profile: Moped Device XDok

Official URL: https://elga.moped.at/StructureDefinition/MopedDeviceXDok | Version: 0.1.0
Draft as of 2026-04-07 | Responsible: ELGA GmbH | Computable Name: MopedDeviceXDok

Moped Definition für XDok

Usages:

- Refer to this Profile: MOPED LKFRequest
- Examples for this Profile: Device/XDokExampleDevice

You can also check for usages in the FHIR IG Statistics

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Key Elements Table
- Differential Table
- Snapshot Table
- Statistics/References
- All

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device | C | 0..* | MopedDevice | Item used in healthcare Constraints: dev-1
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
contained |  | 0..* | Resource | Contained, inline Resources
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored
status | ?!Σ | 1..1 | code | active | inactive | entered-in-error Binding: FHIRDeviceStatus (required): The record status of the device. Required Pattern: active
name | C | 1..* | BackboneElement | The name or names of the device as known to the manufacturer and/or patient
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value | Σ | 1..1 | string | The term that names the device Required Pattern: XDok
type | Σ | 1..1 | code | registered-name | user-friendly-name | patient-reported-name Binding: DeviceNameType (required): The type of name the device is referred by.
display | ?!Σ C | 0..1 | boolean | The preferred device name
category |  | 0..* | CodeableConcept | Indicates a high-level grouping of the device Binding: FHIRDeviceCategory (example): Categories of medical devices. Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/device-category
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: software
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
type |  | 0..* | CodeableConcept | The kind or type of device Binding: Moped Device Types ValueSet (required) Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
version |  | 1..* | BackboneElement | The actual design of the device or software version running on the device
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value |  | 1..1 | string | The version text
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.status | Base | required | FHIR Device Status | 📍5.0.0 | FHIR Std.
Device.name.type | Base | required | Device Name Type | 📍5.0.0 | FHIR Std.
Device.category | Base | example | FHIR Device Category | 📍5.0.0 | FHIR Std.
Device.type | Base | required | Moped Device Types ValueSet | 📦0.1.0 | This IG

#### Constraints

Id | Grade | Path(s) | Description | Expression
dev-1 | error | Device | only one Device.name.display SHALL be true when there is more than one Device.name | `name.where(display=true).count() <= 1`
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().ofType(canonical) | %resource.descendants().ofType(uri) | %resource.descendants().ofType(url))) or descendants().where(reference = '#').exists() or descendants().where(ofType(canonical) = '#').exists() or descendants().where(ofType(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from MopedDevice

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | MopedDevice | Item used in healthcare
status |  | 1..1 | code | active | inactive | entered-in-error Required Pattern: active
name |  |  |  |
value |  | 1..1 | string | The term that names the device Required Pattern: XDok
type |  | 0..* | CodeableConcept | The kind or type of device Required Pattern: At least the following
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
Documentation for this format

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device | C | 0..* | MopedDevice | Item used in healthcare Constraints: dev-1
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: AllLanguages (required): IETF language tag for a human language
Additional Bindings | Purpose
CommonLanguages | Starter
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
displayName |  | 0..1 | string | The name used to display by default when the device is referenced
definition |  | 0..1 | CodeableReference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 1..1 | string | Mandatory fixed portion of UDI
issuer | Σ | 1..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual | card | self-reported | electronic-transmission | unknown Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 1..1 | code | active | inactive | entered-in-error Binding: FHIRDeviceStatus (required): The record status of the device. Required Pattern: active
availabilityStatus |  | 0..1 | CodeableConcept | lost | damaged | destroyed | available Binding: FHIRDeviceAvailabilityStatus (extensible): The availability status reason of the device.
biologicalSourceEvent |  | 0..1 | Identifier | An identifier that supports traceability to the event during which material in this product from one or more biological entities was obtained or pooled
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
name | C | 1..* | BackboneElement | The name or names of the device as known to the manufacturer and/or patient
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value | Σ | 1..1 | string | The term that names the device Required Pattern: XDok
type | Σ | 1..1 | code | registered-name | user-friendly-name | patient-reported-name Binding: DeviceNameType (required): The type of name the device is referred by.
display | ?!Σ C | 0..1 | boolean | The preferred device name
modelNumber |  | 0..1 | string | The manufacturer's model number for the device
partNumber |  | 0..1 | string | The part number or catalog number of the device
category |  | 0..* | CodeableConcept | Indicates a high-level grouping of the device Binding: FHIRDeviceCategory (example): Categories of medical devices. Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/device-category
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: software
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
type |  | 0..* | CodeableConcept | The kind or type of device Binding: Moped Device Types ValueSet (required) Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
version |  | 1..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version, e.g. manufacturer, approved, internal Binding: DeviceVersionType (example): The type of version indicated for the device.
component |  | 0..1 | Identifier | The hardware or software module of the device to which the version applies
installDate |  | 0..1 | dateTime | The date the version was installed on the device
value |  | 1..1 | string | The version text
conformsTo |  | 0..* | BackboneElement | Identifies the standards, specifications, or formal guidances for the capabilities supported by the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
category |  | 0..1 | CodeableConcept | Describes the common type of the standard, specification, or formal guidance. communication | performance | measurement Binding: DeviceSpecificationCategory (example): The kind of standards used by the device.
specification |  | 1..1 | CodeableConcept | Identifies the standard, specification, or formal guidance that the device adheres to Binding: DeviceSpecificationType (example): The type of version indicated for the device.
version |  | 0..1 | string | Specific form or variant of the standard
property |  | 0..* | BackboneElement | Inherent, essentially fixed, characteristics of the device. e.g., time properties, size, material, etc.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property being represented Binding: DeviceType (example): Device property type.
value[x] |  | 1..1 |  | Value of the property
valueQuantity |  |  | Quantity |
valueCodeableConcept |  |  | CodeableConcept |
valueString |  |  | string |
valueBoolean |  |  | boolean |
valueInteger |  |  | integer |
valueRange |  |  | Range |
valueAttachment |  |  | Attachment |
mode |  | 0..1 | CodeableConcept | The designated condition for performing a task Binding: FHIRDeviceOperationMode (example): Operational mode of a device.
cycle |  | 0..1 | Count | The series of occurrences that repeats during the operation of the device
duration |  | 0..1 | Duration | A measurement of time during the device's operation (e.g., days, hours, mins, etc.)
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
endpoint |  | 0..* | Reference(Endpoint) | Technical endpoints providing access to electronic services provided by the device
gateway |  | 0..* | CodeableReference(Device) | Linked device acting as a communication/data collector, translator or controller
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: DeviceSafety (example)
parent |  | 0..1 | Reference(Device) | The higher level or encompassing device that this device is a logical part of
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.language | Base | required | All Languages | 📍5.0.0 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDI Entry Type | 📍5.0.0 | FHIR Std.
Device.status | Base | required | FHIR Device Status | 📍5.0.0 | FHIR Std.
Device.availabilityStatus | Base | extensible | FHIR Device Availability Status | 📍5.0.0 | FHIR Std.
Device.name.type | Base | required | Device Name Type | 📍5.0.0 | FHIR Std.
Device.category | Base | example | FHIR Device Category | 📍5.0.0 | FHIR Std.
Device.type | Base | required | Moped Device Types ValueSet | 📦0.1.0 | This IG
Device.version.type | Base | example | Device Version Type | 📍5.0.0 | FHIR Std.
Device.conformsTo.category | Base | example | Device Specification Category | 📍5.0.0 | FHIR Std.
Device.conformsTo.specification | Base | example | Device Specification Type | 📍5.0.0 | FHIR Std.
Device.property.type | Base | example | Device Property Type | 📍5.0.0 | FHIR Std.
Device.mode | Base | example | FHIR Device Operation Mode | 📍5.0.0 | FHIR Std.
Device.safety | Base | example | Device Safety | 📍5.0.0 | FHIR Std.

#### Constraints

Id | Grade | Path(s) | Description | Expression
dev-1 | error | Device | only one Device.name.display SHALL be true when there is more than one Device.name | `name.where(display=true).count() <= 1`
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().ofType(canonical) | %resource.descendants().ofType(uri) | %resource.descendants().ofType(url))) or descendants().where(reference = '#').exists() or descendants().where(ofType(canonical) = '#').exists() or descendants().where(ofType(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from MopedDevice

Summary

Key Elements View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device | C | 0..* | MopedDevice | Item used in healthcare Constraints: dev-1
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
contained |  | 0..* | Resource | Contained, inline Resources
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored
status | ?!Σ | 1..1 | code | active | inactive | entered-in-error Binding: FHIRDeviceStatus (required): The record status of the device. Required Pattern: active
name | C | 1..* | BackboneElement | The name or names of the device as known to the manufacturer and/or patient
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value | Σ | 1..1 | string | The term that names the device Required Pattern: XDok
type | Σ | 1..1 | code | registered-name | user-friendly-name | patient-reported-name Binding: DeviceNameType (required): The type of name the device is referred by.
display | ?!Σ C | 0..1 | boolean | The preferred device name
category |  | 0..* | CodeableConcept | Indicates a high-level grouping of the device Binding: FHIRDeviceCategory (example): Categories of medical devices. Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/device-category
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: software
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
type |  | 0..* | CodeableConcept | The kind or type of device Binding: Moped Device Types ValueSet (required) Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
version |  | 1..* | BackboneElement | The actual design of the device or software version running on the device
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value |  | 1..1 | string | The version text
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.status | Base | required | FHIR Device Status | 📍5.0.0 | FHIR Std.
Device.name.type | Base | required | Device Name Type | 📍5.0.0 | FHIR Std.
Device.category | Base | example | FHIR Device Category | 📍5.0.0 | FHIR Std.
Device.type | Base | required | Moped Device Types ValueSet | 📦0.1.0 | This IG

#### Constraints

Id | Grade | Path(s) | Description | Expression
dev-1 | error | Device | only one Device.name.display SHALL be true when there is more than one Device.name | `name.where(display=true).count() <= 1`
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().ofType(canonical) | %resource.descendants().ofType(uri) | %resource.descendants().ofType(url))) or descendants().where(reference = '#').exists() or descendants().where(ofType(canonical) = '#').exists() or descendants().where(ofType(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

Differential View

This structure is derived from MopedDevice

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | MopedDevice | Item used in healthcare
status |  | 1..1 | code | active | inactive | entered-in-error Required Pattern: active
name |  |  |  |
value |  | 1..1 | string | The term that names the device Required Pattern: XDok
type |  | 0..* | CodeableConcept | The kind or type of device Required Pattern: At least the following
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
Documentation for this format

Snapshot View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device | C | 0..* | MopedDevice | Item used in healthcare Constraints: dev-1
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: AllLanguages (required): IETF language tag for a human language
Additional Bindings | Purpose
CommonLanguages | Starter
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored
identifier |  | 0..* | Identifier | Instance identifier
displayName |  | 0..1 | string | The name used to display by default when the device is referenced
definition |  | 0..1 | CodeableReference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 1..1 | string | Mandatory fixed portion of UDI
issuer | Σ | 1..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual | card | self-reported | electronic-transmission | unknown Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 1..1 | code | active | inactive | entered-in-error Binding: FHIRDeviceStatus (required): The record status of the device. Required Pattern: active
availabilityStatus |  | 0..1 | CodeableConcept | lost | damaged | destroyed | available Binding: FHIRDeviceAvailabilityStatus (extensible): The availability status reason of the device.
biologicalSourceEvent |  | 0..1 | Identifier | An identifier that supports traceability to the event during which material in this product from one or more biological entities was obtained or pooled
manufacturer |  | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number assigned by the manufacturer
name | C | 1..* | BackboneElement | The name or names of the device as known to the manufacturer and/or patient
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
value | Σ | 1..1 | string | The term that names the device Required Pattern: XDok
type | Σ | 1..1 | code | registered-name | user-friendly-name | patient-reported-name Binding: DeviceNameType (required): The type of name the device is referred by.
display | ?!Σ C | 0..1 | boolean | The preferred device name
modelNumber |  | 0..1 | string | The manufacturer's model number for the device
partNumber |  | 0..1 | string | The part number or catalog number of the device
category |  | 0..* | CodeableConcept | Indicates a high-level grouping of the device Binding: FHIRDeviceCategory (example): Categories of medical devices. Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/device-category
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: software
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
type |  | 0..* | CodeableConcept | The kind or type of device Binding: Moped Device Types ValueSet (required) Required Pattern: At least the following
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
coding |  | 1..* | Coding | Code defined by a terminology system Fixed Value: (Complex)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: https://elga.moped.at/CodeSystem/MopedDeviceTypesCS
version |  | 0..1 | string | Version of the system - if relevant
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: XDok
display |  | 0..1 | string | Representation defined by the system
userSelected |  | 0..1 | boolean | If this coding was chosen directly by the user
text |  | 0..1 | string | Plain text representation of the concept
version |  | 1..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version, e.g. manufacturer, approved, internal Binding: DeviceVersionType (example): The type of version indicated for the device.
component |  | 0..1 | Identifier | The hardware or software module of the device to which the version applies
installDate |  | 0..1 | dateTime | The date the version was installed on the device
value |  | 1..1 | string | The version text
conformsTo |  | 0..* | BackboneElement | Identifies the standards, specifications, or formal guidances for the capabilities supported by the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
category |  | 0..1 | CodeableConcept | Describes the common type of the standard, specification, or formal guidance. communication | performance | measurement Binding: DeviceSpecificationCategory (example): The kind of standards used by the device.
specification |  | 1..1 | CodeableConcept | Identifies the standard, specification, or formal guidance that the device adheres to Binding: DeviceSpecificationType (example): The type of version indicated for the device.
version |  | 0..1 | string | Specific form or variant of the standard
property |  | 0..* | BackboneElement | Inherent, essentially fixed, characteristics of the device. e.g., time properties, size, material, etc.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property being represented Binding: DeviceType (example): Device property type.
value[x] |  | 1..1 |  | Value of the property
valueQuantity |  |  | Quantity |
valueCodeableConcept |  |  | CodeableConcept |
valueString |  |  | string |
valueBoolean |  |  | boolean |
valueInteger |  |  | integer |
valueRange |  |  | Range |
valueAttachment |  |  | Attachment |
mode |  | 0..1 | CodeableConcept | The designated condition for performing a task Binding: FHIRDeviceOperationMode (example): Operational mode of a device.
cycle |  | 0..1 | Count | The series of occurrences that repeats during the operation of the device
duration |  | 0..1 | Duration | A measurement of time during the device's operation (e.g., days, hours, mins, etc.)
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
endpoint |  | 0..* | Reference(Endpoint) | Technical endpoints providing access to electronic services provided by the device
gateway |  | 0..* | CodeableReference(Device) | Linked device acting as a communication/data collector, translator or controller
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device Binding: DeviceSafety (example)
parent |  | 0..1 | Reference(Device) | The higher level or encompassing device that this device is a logical part of
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.language | Base | required | All Languages | 📍5.0.0 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDI Entry Type | 📍5.0.0 | FHIR Std.
Device.status | Base | required | FHIR Device Status | 📍5.0.0 | FHIR Std.
Device.availabilityStatus | Base | extensible | FHIR Device Availability Status | 📍5.0.0 | FHIR Std.
Device.name.type | Base | required | Device Name Type | 📍5.0.0 | FHIR Std.
Device.category | Base | example | FHIR Device Category | 📍5.0.0 | FHIR Std.
Device.type | Base | required | Moped Device Types ValueSet | 📦0.1.0 | This IG
Device.version.type | Base | example | Device Version Type | 📍5.0.0 | FHIR Std.
Device.conformsTo.category | Base | example | Device Specification Category | 📍5.0.0 | FHIR Std.
Device.conformsTo.specification | Base | example | Device Specification Type | 📍5.0.0 | FHIR Std.
Device.property.type | Base | example | Device Property Type | 📍5.0.0 | FHIR Std.
Device.mode | Base | example | FHIR Device Operation Mode | 📍5.0.0 | FHIR Std.
Device.safety | Base | example | Device Safety | 📍5.0.0 | FHIR Std.

#### Constraints

Id | Grade | Path(s) | Description | Expression
dev-1 | error | Device | only one Device.name.display SHALL be true when there is more than one Device.name | `name.where(display=true).count() <= 1`
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().ofType(canonical) | %resource.descendants().ofType(uri) | %resource.descendants().ofType(url))) or descendants().where(reference = '#').exists() or descendants().where(ofType(canonical) = '#').exists() or descendants().where(ofType(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from MopedDevice

Summary

Other representations of profile: CSV, Excel, Schematron