Imaging Diagnostic Report
0.0.1-current - ci-build

Imaging Diagnostic Report, published by IHE Radiology Technical Committee. This guide is not an authorized publication; it is the continuous build for version 0.0.1-current built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/IHE/RAD.IDR/ and changes regularly. See the Directory of published versions

## ValueSet: Imaging Study Endpoint PayloadType Value Set

Official URL: https://profiles.ihe.net/RAD/IDR/ValueSet/imaging-study-endpoint-payloadtype-vs | Version: 0.0.1-current
Draft as of 2024-06-25 | Computable Name: ImagingStudyEndpointPayloadTypeVS

Codes representing the applicable endpoint payloadType to retrieve a study.

References

- ImagingStudy Endpoint

### Logical Definition (CLD)

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM`

  Code | Display
  113014 | Study

### Expansion

Expansion based on codesystem DICOM version2024.2.20240331

This value set contains 1 concepts

Code | System | Display
113014 | http://dicom.nema.org/resources/ontology/DCM | Study

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code