Annuaire Santé
1.1.0 - final-text

Annuaire Santé, published by Agence du Numérique en Santé (ANS) - 2-10 Rue d'Oradour-sur-Glane, 75015 Paris. This guide is not an authorized publication; it is the continuous build for version 1.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/ansforge/IG-fhir-annuaire/ and changes regularly. See the Directory of published versions

## Resource Profile: AS Device Profile

Official URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-device | Version: 1.1.0
Active as of 2025-10-10 | Computable Name: AsDeviceProfile

Profil générique créé à partir de Device dans le contexte de l’Annuaire Santé pour décrire les Equipements Matériels Lourds (EML) mis en place au sein d’un établissement.

Usages:

- Derived from this Profile: AS Donnée Publique Device Profile and AS Donnée Restreinte Device Profile

You can also check for usages in the FHIR IG Statistics

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Differential Table
- Key Elements Table
- Snapshot Table
- Statistics/References
- All

This structure is derived from Device

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
Slices pour extension |  |  |  | Content/Rules for all slices
extension:dateAuthorization |  | 0..1 | Extension | Extension
extension:periodAuthorization |  | 0..1 | Extension | Extension
value[x] |  |  |  |
start |  | 0..1 | dateTime | Date de première mise en œuvre.
end |  | 0..1 | dateTime | Date de fin de mise en œuvre.
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
system |  | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value |  | 0..1 | string | The value that is unique
status |  | 0..1 | code | Le matériel est-il actif ? active | inactive
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
Documentation for this format

#### Terminology Bindings (Differential)

Path | Statut | Usage | ValueSet | Version | Source
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
Slices pour extension |  |  |  | Content/Rules for all slices
extension:dateAuthorization |  | 0..1 | Extension | Extension
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateAuthorization"
extension:periodAuthorization |  | 0..1 | Extension | Extension
extension |  | 0..0 |  |
url |  | 1..1 | uri | "periodAuthorization"
extension:dateUpdateAuthorization |  | 0..1 | Extension | Date de dernière mise à jour de l’autorisation.
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateUpdateAuthorization"
extension:deletedAuthorization |  | 0..1 | Extension | Indicateur de suppression de l'autorisation.
extension |  | 0..0 |  |
url |  | 1..1 | uri | "deletedAuthorization"
url |  | 1..1 | uri | "https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization"
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
system | Σ | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value | Σ | 0..1 | string | The value that is unique Exemple General: 123456
status | ?!Σ | 0..1 | code | Le matériel est-il actif ? active | inactive Binding: FHIRDeviceStatus (required): The availability status of the device.
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
Documentation for this format

#### Terminology Bindings

Path | Statut | Usage | ValueSet | Version | Source
Device.identifier:numAutorisationArhgos.​use | Base | required | IdentifierUse | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Bindings Additionnels | But
AllLanguages | Binding Max
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
id |  | 0..1 | string | Unique id for inter-element referencing
Slices pour extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
extension:dateAuthorization |  | 0..1 | Extension | Extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateAuthorization"
value[x] |  | 0..1 | date | Value of extension
extension:periodAuthorization |  | 0..1 | Extension | Extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "periodAuthorization"
value[x] |  | 0..1 | Period | Value of extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
start | Σ C | 0..1 | dateTime | Date de première mise en œuvre.
end | Σ C | 0..1 | dateTime | Date de fin de mise en œuvre.
extension:dateUpdateAuthorization |  | 0..1 | Extension | Date de dernière mise à jour de l’autorisation.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateUpdateAuthorization"
value[x] |  | 0..1 | date | Value of extension
extension:deletedAuthorization |  | 0..1 | Extension | Indicateur de suppression de l'autorisation.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "deletedAuthorization"
value[x] |  | 0..1 | boolean | Value of extension
url |  | 1..1 | uri | "https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization"
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 0..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
system | Σ | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value | Σ | 0..1 | string | The value that is unique Exemple General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | Le matériel est-il actif ? active | inactive Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Statut | Usage | ValueSet | Version | Source
Device.language | Base | preferred | Common Languages | 📍4.0.1 | FHIR Std.
Device.identifier:numAutorisationArhgos.​use | Base | required | IdentifierUse | 📍4.0.1 | FHIR Std.
Device.identifier:numAutorisationArhgos.​type | Base | extensible | IdentifierType | 📍4.0.1 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDIEntryType | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.statusReason | Base | extensible | FHIRDeviceStatusReason | 📍4.0.1 | FHIR Std.
Device.deviceName.type | Base | required | DeviceNameType | 📍4.0.1 | FHIR Std.
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from Device

Résumé

Mandatory: 0 element(1 nested mandatory element)

Structures

This structure refers to these other structures:

- FR Core Organization Profile (https://hl7.fr/ig/fhir/core/StructureDefinition/fr-core-organization)
- AS Organization Profile (https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-organization)

Extensions

This structure refers to these extensions:

- https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization

Slices

This structure defines the following Slices:

- The element 1 is sliced based on the value of Device.identifier

Differential View

This structure is derived from Device

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
Slices pour extension |  |  |  | Content/Rules for all slices
extension:dateAuthorization |  | 0..1 | Extension | Extension
extension:periodAuthorization |  | 0..1 | Extension | Extension
value[x] |  |  |  |
start |  | 0..1 | dateTime | Date de première mise en œuvre.
end |  | 0..1 | dateTime | Date de fin de mise en œuvre.
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
system |  | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value |  | 0..1 | string | The value that is unique
status |  | 0..1 | code | Le matériel est-il actif ? active | inactive
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
Documentation for this format

#### Terminology Bindings (Differential)

Path | Statut | Usage | ValueSet | Version | Source
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

Key Elements View

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
Slices pour extension |  |  |  | Content/Rules for all slices
extension:dateAuthorization |  | 0..1 | Extension | Extension
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateAuthorization"
extension:periodAuthorization |  | 0..1 | Extension | Extension
extension |  | 0..0 |  |
url |  | 1..1 | uri | "periodAuthorization"
extension:dateUpdateAuthorization |  | 0..1 | Extension | Date de dernière mise à jour de l’autorisation.
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateUpdateAuthorization"
extension:deletedAuthorization |  | 0..1 | Extension | Indicateur de suppression de l'autorisation.
extension |  | 0..0 |  |
url |  | 1..1 | uri | "deletedAuthorization"
url |  | 1..1 | uri | "https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization"
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
system | Σ | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value | Σ | 0..1 | string | The value that is unique Exemple General: 123456
status | ?!Σ | 0..1 | code | Le matériel est-il actif ? active | inactive Binding: FHIRDeviceStatus (required): The availability status of the device.
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
Documentation for this format

#### Terminology Bindings

Path | Statut | Usage | ValueSet | Version | Source
Device.identifier:numAutorisationArhgos.​use | Base | required | IdentifierUse | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

Snapshot View

Nom | Drapeaux | Card. | Type | Description et contraintes Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Bindings Additionnels | But
AllLanguages | Binding Max
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
Slices pour extension |  | 0..* | Extension | Extension Slice: Unordered, Open by value:url
extension:as-ext-authorization |  | 0..1 | (Complex) | AS Authorization Extension URL: https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization
id |  | 0..1 | string | Unique id for inter-element referencing
Slices pour extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
extension:dateAuthorization |  | 0..1 | Extension | Extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateAuthorization"
value[x] |  | 0..1 | date | Value of extension
extension:periodAuthorization |  | 0..1 | Extension | Extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "periodAuthorization"
value[x] |  | 0..1 | Period | Value of extension
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
start | Σ C | 0..1 | dateTime | Date de première mise en œuvre.
end | Σ C | 0..1 | dateTime | Date de fin de mise en œuvre.
extension:dateUpdateAuthorization |  | 0..1 | Extension | Date de dernière mise à jour de l’autorisation.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "dateUpdateAuthorization"
value[x] |  | 0..1 | date | Value of extension
extension:deletedAuthorization |  | 0..1 | Extension | Indicateur de suppression de l'autorisation.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..0 |  |
url |  | 1..1 | uri | "deletedAuthorization"
value[x] |  | 0..1 | boolean | Value of extension
url |  | 1..1 | uri | "https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization"
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices pour identifier |  | 0..* | Identifier | Instance identifier Slice: Unordered, Open by value:system
identifier:numAutorisationArhgos |  | 0..1 | Identifier | Identifiant fonctionnel, numéro d'autorisation ARHGOS (numeroAutorisationARHGOS). Le system est mis à titre indicatif et pourra évoluer.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 0..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
system | Σ | 1..1 | uri | The namespace for the identifier value Required Pattern: https://arhgos.ars.sante.fr
value | Σ | 0..1 | string | The value that is unique Exemple General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | Le matériel est-il actif ? active | inactive Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Marque de l'équipement matériel lourd.
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Numéro de série de l'équipement matériel lourd (numeroSerie).
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type |  | 0..1 | CodeableConcept | Code définissant l'équipement matériel lourd (EML) soumis à autorisation. Binding: JDV_J135-EquipementMaterielLourd-RASS (required)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(FR Core Organization Profile | AS Organization Profile) | Référence vers l'id de la structure FINESS ET à laquelle est rattaché cet équipement matériel lourd (idStructure).
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Statut | Usage | ValueSet | Version | Source
Device.language | Base | preferred | Common Languages | 📍4.0.1 | FHIR Std.
Device.identifier:numAutorisationArhgos.​use | Base | required | IdentifierUse | 📍4.0.1 | FHIR Std.
Device.identifier:numAutorisationArhgos.​type | Base | extensible | IdentifierType | 📍4.0.1 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDIEntryType | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.statusReason | Base | extensible | FHIRDeviceStatusReason | 📍4.0.1 | FHIR Std.
Device.deviceName.type | Base | required | DeviceNameType | 📍4.0.1 | FHIR Std.
Device.type | Base | required | JDV_J135-EquipementMaterielLourd-RASS | 📦1.5.0 | Nomenclatures des objets de santé v1.5

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from Device

Résumé

Mandatory: 0 element(1 nested mandatory element)

Structures

This structure refers to these other structures:

- FR Core Organization Profile (https://hl7.fr/ig/fhir/core/StructureDefinition/fr-core-organization)
- AS Organization Profile (https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-organization)

Extensions

This structure refers to these extensions:

- https://interop.esante.gouv.fr/ig/fhir/annuaire/StructureDefinition/as-ext-authorization

Slices

This structure defines the following Slices:

- The element 1 is sliced based on the value of Device.identifier

Other representations of profile: CSV, Excel, Schematron