Annuaire Santé
1.1.0 - final-text

Annuaire Santé, published by Agence du Numérique en Santé (ANS) - 2-10 Rue d'Oradour-sur-Glane, 75015 Paris. This guide is not an authorized publication; it is the continuous build for version 1.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/ansforge/IG-fhir-annuaire/ and changes regularly. See the Directory of published versions

## Resource Profile: AsDpDeviceProfile - Mappings

Active as of 2025-10-10

Mappings for the as-dp-device resource profile.

#### Mappings to Structures in this Implementation Guide

No Mappings Found

#### Mappings to other Structures

No Mappings Found

#### Other Mappings

Nom | AsDeviceProfile to MOS - EquipementMaterielLourd | RIM Mapping | FiveWs Pattern Mapping | UDI Mapping
--- | --- | --- | --- | ---
Device | EquipementMaterielLourd | Device |  |
id |  |  |  |
meta |  |  |  |
id |  | n/a |  |
Slices pour extension |  | n/a |  |
extension:as-ext-data-trace |  |  |  |
versionId |  |  |  |
lastUpdated |  |  |  |
source |  |  |  |
Slices pour profile |  |  |  |
profile:as-dp-canonical |  |  |  |
security |  |  |  |
tag |  |  |  |
implicitRules |  |  |  |
language |  |  |  |
text |  | Act.text? |  |
contained |  | N/A |  |
Slices pour extension |  |  |  |
extension:as-ext-authorization |  |  |  |
id |  | n/a |  |
Slices pour extension |  | n/a |  |
extension:dateAuthorization | EquipementMaterielLourd.dateDecision |  |  |
id |  | n/a |  |
extension |  |  |  |
url |  | N/A |  |
value[x] |  | N/A |  |
extension:periodAuthorization |  |  |  |
id |  | n/a |  |
extension |  |  |  |
url |  | N/A |  |
value[x] |  | N/A |  |
id |  | n/a |  |
extension |  | n/a |  |
start | EquipementMaterielLourd.datePremierMEO | ./low |  |
end | EquipementMaterielLourd.datefin | ./high |  |
extension:dateUpdateAuthorization |  |  |  |
id |  | n/a |  |
extension |  |  |  |
url |  | N/A |  |
value[x] |  | N/A |  |
extension:deletedAuthorization |  |  |  |
id |  | n/a |  |
extension |  |  |  |
url |  | N/A |  |
value[x] |  | N/A |  |
url |  | N/A |  |
value[x] |  | N/A |  |
modifierExtension |  | N/A |  |
Slices pour identifier |  | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
identifier:numAutorisationArhgos |  | .id | FiveWs.identifier | The serial number which is a component of the production identifier (PI) a conditional variable portion of a UDI. The identifier.type code should be set to “SNO”(Serial Number) and the system left empty.
id |  | n/a |  |
extension |  | n/a |  |
use |  | Role.code or implied by context |  |
type |  | Role.code or implied by context |  |
system |  | II.root or Role.id.root |  |
value | EquipementMaterielLourd.numeroAutorisationARHGOS | II.extension or II.root if system indicates OID or GUID (Or Role.id.extension or root) |  |
period |  | Role.effectiveTime or implied by context |  |
assigner |  | II.assigningAuthorityName but note that this is an improper use by the definition of the field. Also Role.scoper |  |
definition |  |  |  |
udiCarrier |  | .id and .code | FiveWs.identifier |
status |  | .statusCode | FiveWs.status |
statusReason |  |  | FiveWs.status |
distinctIdentifier |  | .lotNumberText | FiveWs.what[x] | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI.
manufacturer | EquipementMaterielLourd.marque | .playedRole[typeCode=MANU].scoper.name | FiveWs.what[x] | N/A
manufactureDate |  | .existenceTime.low | FiveWs.what[x] | The date a specific device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI. For FHIR MM:SS]. If hour is present the minutes and seconds should both be set to “00”.
expirationDate |  | .expirationTime | FiveWs.what[x] | the expiration date of a specific device - which is a component of the production identifier (PI) a conditional variable portion of a UDI. For FHIR MM:SS]. If hour is present the minutes and seconds should both be set to “00”.
lotNumber |  | .lotNumberText | FiveWs.what[x] | The lot or batch number within which a device was manufactured - which is a component of the production identifier (PI) a conditional variable portion of a UDI.
serialNumber | EquipementMaterielLourd.numeroSerie | .playedRole[typeCode=MANU].id | FiveWs.what[x] |
deviceName |  |  |  |
modelNumber |  | .softwareName (included as part) | FiveWs.what[x] |
partNumber |  | .playedRole[typeCode=MANU].id | FiveWs.what[x] |
type | EquipementMaterielLourd.equipementMaterielLourd |  |  |
specialization |  |  |  |
version |  |  |  |
property |  |  |  |
patient |  | .playedRole[typeCode=USED].scoper.playedRole[typeCode=PAT] | FiveWs.subject |
owner |  | .playedRole[typeCode=OWN].scoper | FiveWs.source |
contact |  | .scopedRole[typeCode=CON].player | FiveWs.source |
location |  | .playedRole[typeCode=LOCE].scoper | FiveWs.where[x] |
url |  | .telecom | FiveWs.where[x] |
note |  | .text |  |
safety |  | NA |  |
parent |  |  |  |
Documentation for this format