Mobile Access to DICOM Objects (MADO)
0.1.0-SNAPSHOT - ci-build

Mobile Access to DICOM Objects (MADO), published by IHE Radiology Technical Committee. This guide is not an authorized publication; it is the continuous build for version 0.1.0-SNAPSHOT built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/bvdh/bvdh-ihe-mado/ and changes regularly. See the Directory of published versions

## CodeSystem: MADO Device Type Code System

Official URL: https://profiles.ihe.net/RAD/MADO/CodeSystem/MadoDeviceType | Version: 0.1.0-SNAPSHOT
Standards status: Draft | Maturity Level: 1 | Computable Name: MadoDeviceType

Code system for the type of device used in the MADO context. This code system is used to specify the type of device used in the MADO context, such as the type of device used as the author of an ImagingStudy in the MADO context.

This Code system is referenced in the content logical definition of the following value sets:

- This CodeSystem is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

This code system `https://profiles.ihe.net/RAD/MADO/CodeSystem/MadoDeviceType` defines the following code:

Code | Display | Definition
mado-creator | MADO Creator | Device used to create a FHIR MADO document.