EHDS Logical Information Models
0.2.1 - qa-preview

EHDS Logical Information Models, published by Xt-EHR. This guide is not an authorized publication; it is the continuous build for version 0.2.1 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/costateixeira/xt-ehr-common/ and changes regularly. See the Directory of published versions

## Logical Model: EHDSEndpoint - Detailed Descriptions

Draft as of 2025-12-03

Definitions for the EHDSEndpoint logical model.

- Key Elements Table
- Differential Elements Table
- Snapshot Elements Table

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSEndpoint
Definition | EHDS refined base model for Endpoint Base definition for all types defined in FHIR type system.
Short | Endpoint modelBase for all types and resources
Control | 0..*
Is Modifier | false
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSEndpoint.identifier
Definition | Identifier for the organisation that is used to identify the endpoint across multiple disparate systems.
Short | Identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..*
Type | Identifier
4. EHDSEndpoint.status
Definition | Status of the endpoint. The endpoint status represents whether the endpoint can currently be used for connections or why it can't be used.
Short | Status
Control | 1..1
Binding | hl7:EndpointStatus
Type | CodeableConcept
6. EHDSEndpoint.connectionType
Definition | A coded value that represents the technical details of the usage of this endpoint, such as what WSDLs should be used in what way. (e.g. XDS.b/DICOM/cds-hook).
Short | Connection type
Control | 1..*
Binding | hl7:endpoint-connection-type
Type | CodeableConcept
8. EHDSEndpoint.name
Definition | A friendly name that this endpoint can be referred to with.
Short | Name
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
10. EHDSEndpoint.managingOrganisation
Definition | The organisation that provides technical management services for this endpoint.
Short | Managing organisation
Control | 0..1
Type | http://www.xt-ehr.eu/fhir/models/StructureDefinition/EHDSOrganisation
12. EHDSEndpoint.payload
Definition | The set of payloads that are provided/available at this endpoint.
Short | Payload
Control | 0..*
Type | Base
14. EHDSEndpoint.payload.type
Definition | The type of content that may be used at this endpoint (e.g. XDS Discharge summaries).
Short | Type
Control | 0..*
Binding | hl7:endpoint-payload-type
Type | CodeableConcept
16. EHDSEndpoint.payload.mimeType
Definition | The mime type to send the payload in - e.g. application/fhir+xml, application/fhir+json.
Short | Mime type
Control | 0..*
Binding | BCP-13
Type | CodeableConcept
18. EHDSEndpoint.payload.profileCanonical
Definition | The FHIR profile that is expected at this endpoint. It describes the resources that are handled, or even simply which resource types.
Short | Profile Canonical
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
20. EHDSEndpoint.payload.profileUri
Definition | The profile (as a uri) that is expected at this endpoint when not represented using a FHIR profile.
Short | Profile uri
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
22. EHDSEndpoint.address
Definition | The uri that describes the actual end-point to connect to.
Short | Address
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
24. EHDSEndpoint.header
Definition | Additional headers / information to send as part of the notification. Usage depends on the channel type.
Short | Header
Control | 0..*
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSEndpoint
Definition | EHDS refined base model for Endpoint
Short | Endpoint model
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSEndpoint.identifier
Definition | Identifier for the organisation that is used to identify the endpoint across multiple disparate systems.
Short | Identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..*
Type | Identifier
4. EHDSEndpoint.status
Definition | Status of the endpoint. The endpoint status represents whether the endpoint can currently be used for connections or why it can't be used.
Short | Status
Control | 1..1
Binding | hl7:EndpointStatus
Type | CodeableConcept
6. EHDSEndpoint.connectionType
Definition | A coded value that represents the technical details of the usage of this endpoint, such as what WSDLs should be used in what way. (e.g. XDS.b/DICOM/cds-hook).
Short | Connection type
Control | 1..*
Binding | hl7:endpoint-connection-type
Type | CodeableConcept
8. EHDSEndpoint.name
Definition | A friendly name that this endpoint can be referred to with.
Short | Name
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
10. EHDSEndpoint.managingOrganisation
Definition | The organisation that provides technical management services for this endpoint.
Short | Managing organisation
Control | 0..1
Type | http://www.xt-ehr.eu/fhir/models/StructureDefinition/EHDSOrganisation
12. EHDSEndpoint.payload
Definition | The set of payloads that are provided/available at this endpoint.
Short | Payload
Control | 0..*
Type | Base
14. EHDSEndpoint.payload.type
Definition | The type of content that may be used at this endpoint (e.g. XDS Discharge summaries).
Short | Type
Control | 0..*
Binding | hl7:endpoint-payload-type
Type | CodeableConcept
16. EHDSEndpoint.payload.mimeType
Definition | The mime type to send the payload in - e.g. application/fhir+xml, application/fhir+json.
Short | Mime type
Control | 0..*
Binding | BCP-13
Type | CodeableConcept
18. EHDSEndpoint.payload.profileCanonical
Definition | The FHIR profile that is expected at this endpoint. It describes the resources that are handled, or even simply which resource types.
Short | Profile Canonical
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
20. EHDSEndpoint.payload.profileUri
Definition | The profile (as a uri) that is expected at this endpoint when not represented using a FHIR profile.
Short | Profile uri
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
22. EHDSEndpoint.address
Definition | The uri that describes the actual end-point to connect to.
Short | Address
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
24. EHDSEndpoint.header
Definition | Additional headers / information to send as part of the notification. Usage depends on the channel type.
Short | Header
Control | 0..*
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension

Guidance on how to interpret the contents of this table can be foundhere

0. EHDSEndpoint
Definition | EHDS refined base model for Endpoint
Short | Endpoint model
Control | 0..*
Is Modifier | false
Logical Model | Instances of this logical model are not marked to be the target of a Reference
2. EHDSEndpoint.identifier
Definition | Identifier for the organisation that is used to identify the endpoint across multiple disparate systems.
Short | Identifier
Note | This is a business identifier, not a resource identifier (see discussion)
Control | 1..*
Type | Identifier
4. EHDSEndpoint.status
Definition | Status of the endpoint. The endpoint status represents whether the endpoint can currently be used for connections or why it can't be used.
Short | Status
Control | 1..1
Binding | hl7:EndpointStatus
Type | CodeableConcept
6. EHDSEndpoint.connectionType
Definition | A coded value that represents the technical details of the usage of this endpoint, such as what WSDLs should be used in what way. (e.g. XDS.b/DICOM/cds-hook).
Short | Connection type
Control | 1..*
Binding | hl7:endpoint-connection-type
Type | CodeableConcept
8. EHDSEndpoint.name
Definition | A friendly name that this endpoint can be referred to with.
Short | Name
Control | 0..1
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
10. EHDSEndpoint.managingOrganisation
Definition | The organisation that provides technical management services for this endpoint.
Short | Managing organisation
Control | 0..1
Type | http://www.xt-ehr.eu/fhir/models/StructureDefinition/EHDSOrganisation
12. EHDSEndpoint.payload
Definition | The set of payloads that are provided/available at this endpoint.
Short | Payload
Control | 0..*
Type | Base
14. EHDSEndpoint.payload.type
Definition | The type of content that may be used at this endpoint (e.g. XDS Discharge summaries).
Short | Type
Control | 0..*
Binding | hl7:endpoint-payload-type
Type | CodeableConcept
16. EHDSEndpoint.payload.mimeType
Definition | The mime type to send the payload in - e.g. application/fhir+xml, application/fhir+json.
Short | Mime type
Control | 0..*
Binding | BCP-13
Type | CodeableConcept
18. EHDSEndpoint.payload.profileCanonical
Definition | The FHIR profile that is expected at this endpoint. It describes the resources that are handled, or even simply which resource types.
Short | Profile Canonical
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
20. EHDSEndpoint.payload.profileUri
Definition | The profile (as a uri) that is expected at this endpoint when not represented using a FHIR profile.
Short | Profile uri
Control | 0..*
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
22. EHDSEndpoint.address
Definition | The uri that describes the actual end-point to connect to.
Short | Address
Control | 1..1
Type | uri
Primitive Value | This primitive element may be present, or absent, or replaced by an extension
24. EHDSEndpoint.header
Definition | Additional headers / information to send as part of the notification. Usage depends on the channel type.
Short | Header
Control | 0..*
Type | string
Primitive Value | This primitive element may be present, or absent, or replaced by an extension