HL7 v2.9 Vocabulary
0.2.0 - ci-build

HL7 v2.9 Vocabulary, published by HL7/FO. This guide is not an authorized publication; it is the continuous build for version 0.2.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/frankoemig/hl7.v2.terminology.v29/ and changes regularly. See the Directory of published versions

## CodeSystem: Equipment State Indicator Type Code (2.9 - 1.0.0) (Experimental)

Official URL: http://terminology.hl7.org/v2plusvocab/CodeSystem/equipmentStateIndicator | Version: 1.0.0
Active as of 2026-03-13 | Computable Name: EquipmentStateIndicator
Other Identifiers: OID:2.16.840.1.113883.18.444, urn:ietf:rfc:3986#Uniform Resource Identifier (URI)#http://terminology.hl7.org/v2plusvocab/CodeSystem/v2-0942
Copyright/Legal: HL7 Inc., 2026

HL7-defined code sytem of cocepts that specify the type of measurement of the state of an automated laboratory instrument. Used in HL7 Version 2.x messaging in the INV segment.

This Code system is referenced in the content logical definition of the following value sets:

- Empty_2.16.840.1.113883.21.465

Properties

This code system defines the following properties for its concepts

Name | Code | URI | Type | Description
version introduced | versionIntroduced | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionIntroduced | string | version when was this code introduced
version deprecated | versionDeprecated | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionDeprecated | string | version when was this code deprecated
status | status | http://hl7.org/fhir/concept-properties#status | code | A code that indicates the status of the concept. Typical values are active, experimental, deprecated, and retired
comment, to suppress IG-publisher warning, to be replaced with standard later | comment | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#comment | string | A string that provides additional detail pertinent to the use or understanding of the concept
usage | usage | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#usage | string | usage notes for this code
modified | modified | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#modified | dateTime | date of last modification

Concepts

This case-sensitive code system `http://terminology.hl7.org/v2plusvocab/CodeSystem/equipmentStateIndicator` defines the following codes:

Code | Display | Definition | version introduced | modified
EB | Emergency input buffer current capacity | Current capacity of an emergency input specimen buffer | 2.9 | 2016-03-16
IB | Input buffer current capacity | Current capacity of a regular input specimen buffer | 2.9 | 2016-03-16
IC | Instrument current processing capacity | Current processing capacity of the instrument | 2.9 | 2016-03-16
OB | Output buffer current capacity | Current capacity of an output specimen buffer | 2.9 | 2016-03-16
TA | Current test availability | Current test availability | 2.9 | 2016-03-16