# Supplemental Service Information Values (2.9 - 1.0.0) - HL7 v2.9 Vocabulary v0.1.0

* [**Table of Contents**](toc.md)
* [**Artifacts Summary**](artifacts.md)
* **Supplemental Service Information Values (2.9 - 1.0.0)**

## ValueSet: Supplemental Service Information Values (2.9 - 1.0.0) (Experimental) 

| | |
| :--- | :--- |
| *Official URL*:http://terminology.hl7.org/v2plusvocab/ValueSet/hl7VSsupplementalServiceInformation | *Version*:1.0.0 |
| Active as of 2026-01-27 | *Computable Name*:Hl7VSsupplementalServiceInformation |
| *Other Identifiers:*OID:2.16.840.1.113883.21.477 | |
| **Copyright/Legal**: HL7 Inc., 2026 | |

 
Value Set of codes that specify a kind of supplemental service information sent between a placer system and a filler system for the universal procedure code reported in OBR-4 Universal Service ID. This specifies ordering information detail that is not available in other specific tables for fields in the OBR segment. These might be details such as whether a study is to be done on the right or left, for example, where the study is of the arm and the order master file does not distinguish right from left, or whether a study is to be done with or without contrast (when the order master file does not make such distinctions). 

 **References** 

This value set is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

### Logical Definition (CLD)

 

### Expansion

No Expansion for this valueset (not supported by Publication Tooling)

-------

 Explanation of the columns that may appear on this page: 

| | |
| :--- | :--- |
| Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies |
| System | The source of the definition of the code (when the value set draws in codes defined elsewhere) |
| Code | The code (used as the code in the resource instance) |
| Display | The display (used in the*display*element of a[Coding](http://hl7.org/fhir/R4/datatypes.html#Coding)). If there is no display, implementers should not simply display the code, but map the concept into their application |
| Definition | An explanation of the meaning of the concept |
| Comments | Additional notes about how to use the code |



## Resource Content

```json
{
  "resourceType" : "ValueSet",
  "id" : "hl7VSsupplementalServiceInformation",
  "url" : "http://terminology.hl7.org/v2plusvocab/ValueSet/hl7VSsupplementalServiceInformation",
  "identifier" : [
    {
      "system" : "urn:ietf:rfc:3986",
      "value" : "urn:oid:2.16.840.1.113883.21.477"
    }
  ],
  "version" : "1.0.0",
  "name" : "Hl7VSsupplementalServiceInformation",
  "title" : "Supplemental Service Information Values (2.9 - 1.0.0)",
  "status" : "active",
  "experimental" : true,
  "date" : "2026-01-27T19:46:43+00:00",
  "publisher" : "HL7/FO",
  "contact" : [
    {
      "name" : "HL7/FO",
      "telecom" : [
        {
          "system" : "url",
          "value" : "http://www.hl7.org"
        }
      ]
    }
  ],
  "description" : "Value Set of codes that specify a kind of supplemental service information sent between a placer system and a filler system for the universal procedure code reported in OBR-4 Universal Service ID. This specifies ordering information detail that is not available in other specific tables for fields in the OBR segment.  These might be details such as whether a study is to be done on the right or left, for example, where the study is of the arm and the order master file does not distinguish right from left, or whether a study is to be done with or without contrast (when the order master file does not make such distinctions).",
  "copyright" : "HL7 Inc., 2026",
  "compose" : {
    "include" : [
      {
        "system" : "http://terminology.hl7.org/v2plusvocab/CodeSystem/supplementalServiceInformation",
        "version" : "1"
      }
    ]
  }
}

```
