HL7 v2.9 Vocabulary
0.1.0 - ci-build

HL7 v2.9 Vocabulary, published by HL7/FO. This guide is not an authorized publication; it is the continuous build for version 0.1.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/frankoemig/hl7.v2.terminology.v29/ and changes regularly. See the Directory of published versions

## CodeSystem: Cycle Type (2.9 - 1.0.1) (Experimental)

Official URL: http://terminology.hl7.org/v2plusvocab/CodeSystem/cycleType | Version: 1.0.1
Active as of 2026-01-27 | Computable Name: CycleType
Other Identifiers: OID:2.16.840.1.113883.18.387
Copyright/Legal: HL7 Inc., 2026

Code system of concepts specifying the type of cycle that is being executed. A cycle type is a specific sterilization method used for a specific type of supply item. Used in HL7 Version 2.x messaging in the SCD segment.

This Code system is referenced in the content logical definition of the following value sets:

- Hl7VScycleType

Properties

This code system defines the following properties for its concepts

Name | Code | URI | Type | Description
versionIntroduced | versionIntroduced | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionIntroduced | string | version when was this code introduced
versionDeprecated | versionDeprecated | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionDeprecated | string | version when was this code deprecated
status | status | http://hl7.org/fhir/concept-properties#status | code | A code that indicates the status of the concept. Typical values are active, experimental, deprecated, and retired
comment | comment | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#comment | string | A string that provides additional detail pertinent to the use or understanding of the concept
usage | usage | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#usage | string | usage notes for this code
modified | modified | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#modified | dateTime | date of last modification

Concepts

This case-sensitive code system `http://terminology.hl7.org/v2plusvocab/CodeSystem/cycleType` defines the following codes:

Code | Display | Definition | versionIntroduced | comment | modified
2RS | Second Rinse | Second Rinse | 2.6 |  | 2015-07-13
ANR | Anesthesia/Respiratory | Anesthesia/Respiratory | 2.6 | Special Wash cycle | 2015-07-13
BDP | Bedpans | Bedpans | 2.6 |  | 2015-07-13
BWD | Bowie-Dick Test | Bowie-Dick Test | 2.6 | A Bowie-Dick test cycle is a special cycle used to test the integrity of the sterilizer chamber to hold a vacuum. | 2015-07-13
CMW | Chemical Wash | Chemical Wash | 2.6 | A chemical wash cycle. | 2015-07-13
COD | Code | Code | 2.6 |  | 2015-07-13
CRT | Cart Wash | Cart Wash | 2.6 |  | 2015-07-13
DEC | Decontamination | Decontamination | 2.6 |  | 2015-07-13
DRT | Dart | Dart | 2.6 | A dart cycle is a special cycle used to test the integrity of the sterilizer chamber to hold a vacuum. | 2015-07-13
DRW | Dart Warm-up Cycle | Dart Warm-up Cycle | 2.6 | A dart warm-up cycle is used to bring the sterilizer chamber up to operating temperature in order to run a dart test cycle. | 2015-07-13
EOH | EO High Temperature | EO High Temperature | 2.6 |  | 2015-07-13
EOL | EO Low Temperature | EO Low Temperature | 2.6 |  | 2015-07-13
EXP | Express | Express | 2.6 | An express cycle is similar to a flash cycle but the supply item is wrapped. | 2015-07-13
FLS | Flash | Flash | 2.6 | Used to quickly sterilize instruments that were dropped during surgery. | 2015-07-13
GLS | Glassware | Glassware | 2.6 |  | 2015-07-13
GNP | Gen. Purpose | Gen. Purpose | 2.6 |  | 2015-07-13
GRV | Gravity | Gravity | 2.6 | A gravity cycle is executed at atmospheric pressure. | 2015-07-13
GTL | Gentle | Gentle | 2.6 |  | 2015-07-13
ISO | Isothermal | Isothermal | 2.6 |  | 2015-07-13
IST | Instrument Wash | Instrument Wash | 2.6 |  | 2015-07-13
LKT | Leak Test | Leak Test | 2.6 | A leak test cycle tests the integrity of the sterilizer chamber to hold a vacuum over a specific period of time. | 2015-07-13
LQD | Liquid | Liquid | 2.6 | A cycle specific to sterilizing liquids. | 2015-07-13
OPW | Optional Wash | Optional Wash | 2.6 | Any Optional Wash cycle | 2015-07-13
PEA | Peracetic Acid | Peracetic Acid | 2.6 | A peracetic acid cycle. | 2015-07-13
PLA | Plastic Goods Wash | Plastic Goods Wash | 2.6 |  | 2015-07-13
PRV | Prevac | Prevac | 2.6 | A prevac cycle is vacuum assisted. | 2015-07-13
RNS | Rinse | Rinse | 2.6 |  | 2015-07-13
SFP | Steam Flush Pressure Pulse | Steam Flush Pressure Pulse | 2.6 | An SFPP cycle uses steam pulses instead of a vacuum during the conditioning phase of the cycle when the supply item is wrapped. | 2015-07-13
THR | Thermal | Thermal | 2.6 |  | 2015-07-13
TRB | Tray/Basin | Tray/Basin | 2.6 |  | 2015-07-13
UTL | Utensil Wash | Utensil Wash | 2.6 |  | 2015-07-13
WFP | Wrap/Steam Flush Pressure Pulse (Wrap/SFPP) | Wrap/Steam Flush Pressure Pulse (Wrap/SFPP) | 2.6 | A Wrap/SFPP cycle uses steam pulses instead of a vacuum during the conditioning phase of the cycle when the supply item is unwrapped. | 2015-07-13