PanCareSurPass Project HL7 FHIR Implementation Guide
1.0.0 - release 150

PanCareSurPass Project HL7 FHIR Implementation Guide, published by PanCareSurPass Project. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/hl7-eu/pcsp/ and changes regularly. See the Directory of published versions

## ValueSet: Radiotherapy Dose Type

Official URL: http://hl7.eu/fhir/ig/pcsp/ValueSet/vs-radiotherapyDoseType-eu-pcsp | Version: 1.0.0
Active as of 2026-01-16 | Computable Name: RadiotherapyDoseTypeVs

Types of radiotherapy cumulative dose this procedure is referring to

References

- Observation: Radiotherapy Total Dose PCSP

### Logical Definition (CLD)

This value set includes codes based on the following rules:

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM` version 📦01

  Code | Display | Definition
  113725 | Dose (RP) Total | Total Dose related to Reference Point (RP). (in the scope of the including report)

- Include these codes as defined in `http://snomed.info/sct` version Not Stated (use latest from terminology server)

  Code | Display
  445565002 | Total boost radiation dose delivered
  445461008 | Total radiation dose delivered

### Expansion

Expansion performed internally based on:

- codesystem DICOM Controlled Terminology Definitions v01 (CodeSystem)
- SNOMED CT International edition 01-Sep 2023

This value set contains 3 concepts

System | Code | Display (en) | Definition | JSON | XML
`http://dicom.nema.org/resources/ontology/DCM` | 113725 | Dose (RP) Total | Total Dose related to Reference Point (RP). (in the scope of the including report) |  |
`http://snomed.info/sct` | 445565002 | Total boost radiation dose delivered (observable entity) |  |  |
`http://snomed.info/sct` | 445461008 | Total radiation dose delivered (observable entity) |  |  |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
System | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code