AU Base Implementation Guide
6.0.0-ci-build - CI Build

AU Base Implementation Guide, published by HL7 Australia. This guide is not an authorized publication; it is the continuous build for version 6.0.0-ci-build built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/hl7au/au-fhir-base/ and changes regularly. See the Directory of published versions

## CodeSystem: Communication Request Reason

Official URL: http://terminology.hl7.org.au/CodeSystem/communicationrequest-reason | Version: 6.0.0-ci-build
Standards status: Deprecated | Maturity Level: 1 | Computable Name: CommunicationRequestReason
Copyright/Legal: HL7 Australia© 2018+; Licensed Under Creative Commons No Rights Reserved.

The Communication Request Reason code system defines concepts that represent the reason codes for a communication request.

This code system is deprecated in AU Base as work undertaken in the AU eRequesting project does no longer require these concepts for differentiating communication request reasons.

### Usage Notes

This Code system is referenced in the content logical definition of the following value sets:

- This CodeSystem is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

Changes since version 5.0.0:

- New Content

Profile: `https://healthterminologies.gov.au/fhir/StructureDefinition/complete-code-system-4`

This case-sensitive code system `http://terminology.hl7.org.au/CodeSystem/communicationrequest-reason` defines the following codes:

Code | Display | Definition
urgent | Urgent Results | A request for results to be communicated urgently to the nominated recipient.
patient | Patient Request | A patient's request about receiving communication from a service provider.
copyto | Copy To | A request for results to be copied to an additional recipient.