DK EHMI Endpoint Register (EER) - Configurations
1.0.1-draft - ci-build

DK EHMI Endpoint Register (EER) - Configurations, published by MedCom. This guide is not an authorized publication; it is the continuous build for version 1.0.1-draft built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/medcomdk/dk-ehmi-eer-configurations/ and changes regularly. See the Directory of published versions

## Example Endpoint: 5790000127528

Profile: EER Endpoint - General for Messaging

identifier: GLN/5790000127528

status: Suspended

connectionType: EHMI Endpoint Register (EER) - Connection Types CS: EerMessagingEdelivery (EHMI messaging via eDelivery)

name: EER Messaging Endpoint - LægerneMereteAndersenogDorteLeiKaltoft.8240.Risskov.753691000016000 FHIR Endpoint

managingOrganization: Organization Lægerne Merete Andersen og Dorte Lei Kaltoft (753691000016000)

period: 2021-07-07 00:00:00+0200 --> (ongoing)

payloadType: HomeCareObservation 1.2, Acknowledgement 2.0, ehmiSBDH Acknowledgement 1.0

payloadMimeType: text/xml, application/fhir+xml, application/fhir+json

address: https://example.org/fhir