DK EHMI Endpoint Register (EER) - Configurations
1.0.0-draft - ci-build

DK EHMI Endpoint Register (EER) - Configurations, published by MedCom. This guide is not an authorized publication; it is the continuous build for version 1.0.0-draft built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/medcomdk/dk-ehmi-eer-configurations/ and changes regularly. See the Directory of published versions

## Example Endpoint: DigitalSundhedDanmark-EerEndpointMessaging-eDelivery-DDS-TEST1

Profile: EER Endpoint - General for Messaging

EER System Extension - MSH: Device: identifier = NSPMSH-test-DDS; status = active; manufacturer = KvalitetsIT; type = Message Service Handler

EER System Extension - AP: Device: identifier = NSPAP-test-DDS; status = active; manufacturer = KvalitetsIT; type = eDelivery Access Point

identifier: `https://www.gs1.org/gln`/5790002515811

status: Active

connectionType: EHMI Endpoint Register (EER) - Connection Types CS: EerMessagingEdelivery (EHMI messaging via eDelivery)

name: DigitalSundhedDanmark-EerEndpointMessaging-eDelivery-eDelivery-DDS-TEST1

managingOrganization: Organization DigitalSundhedDanmark-Organization-eDelivery (1134981000016000)

period: 2026-01-01 --> (ongoing)

payloadType: HomeCareObservation 1.1

payloadMimeType: text/xml, application/fhir+xml, application/fhir+json

address: http://www.dsd-dds.dk/dds-test1