DK EHMI Endpoint Register (EER) - Configurations
1.0.0-draft - ci-build

DK EHMI Endpoint Register (EER) - Configurations, published by MedCom. This guide is not an authorized publication; it is the continuous build for version 1.0.0-draft built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/medcomdk/dk-ehmi-eer-configurations/ and changes regularly. See the Directory of published versions

## Example Endpoint: EER Messaging Endpoint - LaegerneStjernepladsen.8200.AarhusN.5790002401428

Profile: EER Endpoint - General for Messaging

EER System Extension - MSH: Device: identifier = MultiMedMSH-prod-LPS; status = active; manufacturer = MultiMed; type = Message Service Handler

EER System Extension - AP: Device: identifier = MultiMedAP-prod-LPS; status = active; manufacturer = MultiMed; type = eDelivery Access Point

identifier: `https://www.gs1.org/gln`/5790002401428

status: Active

connectionType: [not stated]: EerMessagingEdelivery (EerMessagingEdelivery)

name: EER Messaging Endpoint - LaegerneStjernepladsen.8200.AarhusN.5790002401428 FHIR Endpoint

managingOrganization: Organization Lægerne Stjernepladsen I/S

period: 2025-01-01 --> (ongoing)

payloadType: HomeCareObservation 1.0, Acknowledgement 2.0, SBDH Ack 1.0

payloadMimeType: text/xml, application/fhir+xml, application/fhir+json

address: https://example.org/fhir