Radiation Dose Summary for Diagnostic Procedures on FHIR
1.0.0 -

Radiation Dose Summary for Diagnostic Procedures on FHIR, published by HL7 International / Imaging Integration. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/fhir-radiation-dose-summary-ig/ and changes regularly. See the Directory of published versions

## : DICOM Identifier Type

Page standards status: Trial-use | Maturity Level: 2

Raw xml | Download

    <CodeSystem xmlns="http://hl7.org/fhir">
      <id value="dicom-identifier-type"/>
      <language value="en"/>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: CodeSystem dicom-identifier-type</b></p><a name="dicom-identifier-type"> </a><a name="hcdicom-identifier-type"> </a><p>This case-sensitive code system <code>http://hl7.org/fhir/uv/radiation-dose-summary/CodeSystem/dicom-identifier-type</code> defines the following codes in a Is-A hierarchy:</p><table class="codes"><tr><td style="white-space:nowrap"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style="white-space:nowrap">irradiation-event-uid<a name="dicom-identifier-type-irradiation-event-uid"> </a></td><td>Irradiation Event UID</td><td>Unique identification of the irradiation event</td></tr><tr><td style="white-space:nowrap">device-serial-number<a name="dicom-identifier-type-device-serial-number"> </a></td><td>Device Serial Number</td><td>Manufacturer's serial number of the device</td></tr><tr><td style="white-space:nowrap">application-entity<a name="dicom-identifier-type-application-entity"> </a></td><td>Application Entity</td><td>Title of a DICOM Application Entity</td></tr><tr><td style="white-space:nowrap">device-uid<a name="dicom-identifier-type-device-uid"> </a></td><td>Device UID</td><td>Unique identifier of the equipment that produced the Composite Instances</td></tr><tr><td style="white-space:nowrap">device-id<a name="dicom-identifier-type-device-id"> </a></td><td>Device ID</td><td>User-supplied identifier for the device</td></tr><tr><td style="white-space:nowrap">study-instance-uid<a name="dicom-identifier-type-study-instance-uid"> </a></td><td>Study Instance UID</td><td>Unique identifier for the Study</td></tr><tr><td style="white-space:nowrap">sop-instance-uid<a name="dicom-identifier-type-sop-instance-uid"> </a></td><td>SOP Instance UID</td><td>Uniquely identifies the SOP Instance</td></tr></table></div>
      </text>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-wg">
        <valueCode value="ii"/>
      </extension>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm">
        <valueInteger value="2">
          <extension
                     url="http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom">
            <valueCanonical
                            value="http://hl7.org/fhir/uv/radiation-dose-summary/ImplementationGuide/hl7.fhir.uv.radiation-dose-summary"/>
          </extension>
        </valueInteger>
      </extension>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status">
        <valueCode value="trial-use">
          <extension
                     url="http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom">
            <valueCanonical
                            value="http://hl7.org/fhir/uv/radiation-dose-summary/ImplementationGuide/hl7.fhir.uv.radiation-dose-summary"/>
          </extension>
        </valueCode>
      </extension>
      <url
           value="http://hl7.org/fhir/uv/radiation-dose-summary/CodeSystem/dicom-identifier-type"/>
      <version value="1.0.0"/>
      <name value="DicomIdentifierType"/>
      <title value="DICOM Identifier Type"/>
      <status value="active"/>
      <experimental value="false"/>
      <date value="2025-10-29T17:37:08+00:00"/>
      <publisher value="HL7 International / Imaging Integration"/>
      <contact>
        <telecom>
          <system value="url"/>
          <value value="http://www.hl7.org/Special/committees/imagemgt"/>
        </telecom>
      </contact>
      <contact>
        <name value="HL7 Imaging Integration Workgroup"/>
        <telecom>
          <system value="url"/>
          <value value="http://www.hl7.org/Special/committees/imagemgt"/>
        </telecom>
      </contact>
      <contact>
        <name value="Abderrazek Boufahja"/>
        <telecom>
          <system value="email"/>
          <value value="abderrazek.boufahja@gehealthcare.com"/>
        </telecom>
      </contact>
      <description value="Identifier types related to DICOM UIDs"/>
      <jurisdiction>
        <coding>
          <system value="http://unstats.un.org/unsd/methods/m49/m49.htm"/>
          <code value="001"/>
        </coding>
      </jurisdiction>
      <copyright
                 value="These codes are derived from Digital Imaging and Communications in Medicine (DICOM) Standard, Part 6: Data Dictionary, Copyright &amp;#xA9; 2025 by the National Electrical Manufacturers Association."/>
      <caseSensitive value="true"/>
      <hierarchyMeaning value="is-a"/>
      <content value="complete"/>
      <count value="7"/>
      <concept>
        <code value="irradiation-event-uid"/>
        <display value="Irradiation Event UID"/>
        <definition value="Unique identification of the irradiation event"/>
      </concept>
      <concept>
        <code value="device-serial-number"/>
        <display value="Device Serial Number"/>
        <definition value="Manufacturer's serial number of the device"/>
      </concept>
      <concept>
        <code value="application-entity"/>
        <display value="Application Entity"/>
        <definition value="Title of a DICOM Application Entity"/>
      </concept>
      <concept>
        <code value="device-uid"/>
        <display value="Device UID"/>
        <definition
                    value="Unique identifier of the equipment that produced the Composite Instances"/>
      </concept>
      <concept>
        <code value="device-id"/>
        <display value="Device ID"/>
        <definition value="User-supplied identifier for the device"/>
      </concept>
      <concept>
        <code value="study-instance-uid"/>
        <display value="Study Instance UID"/>
        <definition value="Unique identifier for the Study"/>
      </concept>
      <concept>
        <code value="sop-instance-uid"/>
        <display value="SOP Instance UID"/>
        <definition value="Uniquely identifies the SOP Instance"/>
      </concept>
    </CodeSystem>