Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Heart Rate Numeric metric example - XML Representation

Raw xml | Download

    <DeviceMetric xmlns="http://hl7.org/fhir">
      <id value="HeartRateNumericDeviceMetric"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"/>
      </meta>
      <text>
        <status value="extensions"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p><b>Generated Narrative: DeviceMetric</b><a name="HeartRateNumericDeviceMetric"> </a></p><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px">Resource DeviceMetric &quot;HeartRateNumericDeviceMetric&quot; </p><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-NumericDeviceMetric.html">Numeric DeviceMetric profile</a></p></div><blockquote><p><b>Relation extension</b></p><blockquote><p><b>url</b></p><code>kind</code></blockquote><p><b>value</b>: DCE</p><blockquote><p><b>url</b></p><code>entries</code></blockquote><p><b>value</b>: <a href="DeviceMetric-ECGSampleArrayDeviceMetric.html">DeviceMetric/ECGSampleArrayDeviceMetric</a></p></blockquote><blockquote><p><b>Technical range extension</b></p><blockquote><p><b>url</b></p><code>lowerLimit</code></blockquote><p><b>value</b>: 0</p><blockquote><p><b>url</b></p><code>upperLimit</code></blockquote><p><b>value</b>: 200</p><blockquote><p><b>url</b></p><code>stepWidth</code></blockquote><p><b>value</b>: 1</p><blockquote><p><b>url</b></p><code>relativeAccuracy</code></blockquote><p><b>value</b>: 0.01</p><blockquote><p><b>url</b></p><code>absoluteAccuracy</code></blockquote><p><b>value</b>: 0.01</p></blockquote><p><b>type</b>: HR <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#147842 &quot;MDC_ECG_HEART_RATE&quot;)</span></p><p><b>unit</b>: bpm <span style="background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki"> (<a href="http://terminology.hl7.org/5.0.0/CodeSystem-v3-mdc.html">ISO 11073-10101 Health informatics - Point-of-care</a>#264864 &quot;MDC_DIM_BEAT_PER_MIN&quot;)</span></p><p><b>source</b>: <a href="Device-PhysioMonitorMdsDevice.html">Device/PhysioMonitorMdsDevice</a></p><p><b>parent</b>: <a href="Device-HeartRateChannelDevice.html">Device/HeartRateChannelDevice</a></p><p><b>operationalStatus</b>: on</p><p><b>color</b>: green</p><p><b>category</b>: measurement</p></div>
      </text>
      <extension url="http://hl7.org/fhir/uv/pocd/StructureDefinition/relation">
        <extension url="kind">
          <valueCode value="DCE"/>
        </extension>
        <extension url="entries">
          <valueReference>
            <reference value="DeviceMetric/ECGSampleArrayDeviceMetric"/>
          </valueReference>
        </extension>
      </extension>
      <extension
                 url="http://hl7.org/fhir/uv/pocd/StructureDefinition/technical-range">
        <extension url="lowerLimit">
          <valueDecimal value="0"/>
        </extension>
        <extension url="upperLimit">
          <valueDecimal value="200"/>
        </extension>
        <extension url="stepWidth">
          <valueDecimal value="1"/>
        </extension>
        <extension url="relativeAccuracy">
          <valueDecimal value="0.01"/>
        </extension>
        <extension url="absoluteAccuracy">
          <valueDecimal value="0.01"/>
        </extension>
      </extension>
      <type>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="147842"/>
          <display value="MDC_ECG_HEART_RATE"/>
        </coding>
        <text value="HR"/>
      </type>
      <unit>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="264864"/>
          <display value="MDC_DIM_BEAT_PER_MIN"/>
        </coding>
        <text value="bpm"/>
      </unit>
      <source>
        <reference value="Device/PhysioMonitorMdsDevice"/>
      </source>
      <parent>
        <reference value="Device/HeartRateChannelDevice"/>
      </parent>
      <operationalStatus value="on"/>
      <color value="green"/>
      <category value="measurement"/>
    </DeviceMetric>