Point-of-Care Device Implementation Guide
current - CI Build

Point-of-Care Device Implementation Guide, published by HL7 International - Devices Work Group. This is not an authorized publication; it is the continuous build for version current). This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## CodeSystem: Kind of relation code system

Official URL: http://hl7.org/fhir/uv/pocd/CodeSystem/kind-of-relation | Version: current
Draft as of 2020-05-12 | Computable Name: Kind

CodeSystem for IEEE 11073-10207 Relation/Kind

This Code system is referenced in the content logical definition of the following value sets:

- Kind

This code system `http://hl7.org/fhir/uv/pocd/CodeSystem/kind-of-relation` defines the following codes:

Code | Display | Definition
Rcm | Recommendation | The METRIC is a recommendation for the containment tree entries defined in ./pm:Relation/@Entries
PS | Presetting | Presetting. This METRIC is a presetting for the containment tree entries defined in ./pm:Relation/@Entries.
SST | Set of summary statistics | The METRIC is part of a set of summary statistics for a sample where other METRICs that belong to the summary statistics are defined in ./pm:Relation/@Entries.
ECE | Effect on containment tree entries | When changed, the METRIC has an effect on the containment tree entries defined in ./pm:Relation/@Entries. If Kind is ECE, ./pm:Relation/pm:Code SHOULD be set to classify the effect.
DCE | Derived from containment tree entries | The METRIC is derived from the containment tree entries defined in ./pm:Relation/@Entries. If Kind is DCE, ./pm:Relation/pm:Code MAY be set to classify the form of derivation.
Oth | Other | Relation is specified by other means, e.g., ./pm:Relation/pm:Code or extension element.