Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Measurement status codes - XML Representation

Page standards status: Trial-use | Maturity Level: 2

Raw xml | Download

    <CodeSystem xmlns="http://hl7.org/fhir">
      <id value="measurement-status"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/StructureDefinition/shareablecodesystem"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: CodeSystem measurement-status</b></p><a name="measurement-status"> </a><a name="hcmeasurement-status"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="http://hl7.org/fhir/R4/shareablecodesystem.html">Shareable CodeSystem</a></p></div><p>This case-insensitive code system <code>http://terminology.hl7.org/CodeSystem/measurement-status</code> defines the following codes:</p><table class="codes"><tr><td style="white-space:nowrap"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style="white-space:nowrap">questionable<a name="measurement-status-questionable"> </a></td><td>Questionable</td><td>Data may not be reliable</td></tr><tr><td style="white-space:nowrap">calibration-ongoing<a name="measurement-status-calibration-ongoing"> </a></td><td>Calibration ongoing</td><td>Calibration is ongoing</td></tr><tr><td style="white-space:nowrap">validated-data<a name="measurement-status-validated-data"> </a></td><td>Validated data</td><td>Relevant, e.g., in an archive</td></tr><tr><td style="white-space:nowrap">early-indication<a name="measurement-status-early-indication"> </a></td><td>Early indication</td><td>Early estimate of value</td></tr><tr><td style="white-space:nowrap">msmt-ongoing<a name="measurement-status-msmt-ongoing"> </a></td><td>Measurement ongoing</td><td>Indicates that a new measurement is just being taken</td></tr><tr><td style="white-space:nowrap">in-alarm<a name="measurement-status-in-alarm"> </a></td><td>Measurement in alarm</td><td>Measurement has an active alarm condition</td></tr><tr><td style="white-space:nowrap">alarm-inhibited<a name="measurement-status-alarm-inhibited"> </a></td><td>Measurement alarms inhibited</td><td>Measurement supports alarming and alarms are turned off</td></tr></table></div>
      </text>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-wg">
        <valueCode value="dev"/>
      </extension>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm">
        <valueInteger value="2">
          <extension
                     url="http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom">
            <valueCanonical
                            value="http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"/>
          </extension>
        </valueInteger>
      </extension>
      <extension
                 url="http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status">
        <valueCode value="trial-use">
          <extension
                     url="http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom">
            <valueCanonical
                            value="http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"/>
          </extension>
        </valueCode>
      </extension>
      <url value="http://terminology.hl7.org/CodeSystem/measurement-status"/>
      <version value="1.0.0"/>
      <name value="MeasurementStatus"/>
      <title value="Measurement status codes"/>
      <status value="active"/>
      <experimental value="false"/>
      <date value="2019-09-28"/>
      <publisher value="HL7 International / Devices"/>
      <contact>
        <telecom>
          <system value="url"/>
          <value value="http://www.hl7.org/Special/committees/healthcaredevices"/>
        </telecom>
      </contact>
      <description
                   value="Measurement status definitions from the ISO/IEEE 11073-10201 DIM. This CodeSystem is intended to be part of THO (terminology.hl7.org) and the URL already assumes that."/>
      <jurisdiction>
        <coding>
          <system value="http://unstats.un.org/unsd/methods/m49/m49.htm"/>
          <code value="001"/>
        </coding>
      </jurisdiction>
      <caseSensitive value="false"/>
      <content value="complete"/>
      <concept>
        <code value="questionable"/>
        <display value="Questionable"/>
        <definition value="Data may not be reliable"/>
      </concept>
      <concept>
        <code value="calibration-ongoing"/>
        <display value="Calibration ongoing"/>
        <definition value="Calibration is ongoing"/>
      </concept>
      <concept>
        <code value="validated-data"/>
        <display value="Validated data"/>
        <definition value="Relevant, e.g., in an archive"/>
      </concept>
      <concept>
        <code value="early-indication"/>
        <display value="Early indication"/>
        <definition value="Early estimate of value"/>
      </concept>
      <concept>
        <code value="msmt-ongoing"/>
        <display value="Measurement ongoing"/>
        <definition value="Indicates that a new measurement is just being taken"/>
      </concept>
      <concept>
        <code value="in-alarm"/>
        <display value="Measurement in alarm"/>
        <definition value="Measurement has an active alarm condition"/>
      </concept>
      <concept>
        <code value="alarm-inhibited"/>
        <display value="Measurement alarms inhibited"/>
        <definition
                    value="Measurement supports alarming and alarms are turned off"/>
      </concept>
    </CodeSystem>