Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : CVP Sample Array observation example - XML Representation

Page standards status: Informative

Raw xml | Download

    <Observation xmlns="http://hl7.org/fhir">
      <id value="CVPSampleArrayObservation"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/SampleArrayObservation"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: Observation CVPSampleArrayObservation</b></p><a name="CVPSampleArrayObservation"> </a><a name="hcCVPSampleArrayObservation"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-SampleArrayObservation.html">Sample Array Observation profile</a></p></div><p><b>status</b>: Final</p><p><b>code</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 150084}">MDC_PRESS_BLD_VEN_CENT</span></p><p><b>subject</b>: <a href="Patient-SomePatient.html">John Doe  Male, DoB: 1967-05-04 ( Medical record number)</a></p><p><b>effective</b>: 2021-07-09 11:33:23+0200 --&gt; 2021-07-09 11:33:24+0200</p><p><b>value</b>: Origin: 0 mmHg , Dimensions: 1 , Data: 2.00 2.00 2.00 2.01 2.02 2.03 2.06 2.09 2.13 2.19 2.25 2.33 2.42 2.53 2.65 2.78 2.93 3.09 3.27 3.47 3.68 3.90 4.14 4.40 4.67 4.96 5.34 5.82 6.37 6.90 7.35 7.68 7.89 7.98 8.00 7.94 7.82 7.64 7.41 7.14 6.84 6.48 6.11 5.85 5.73 5.79 5.95 6.22 6.45 6.54 6.56 6.44 6.20 5.88 5.48 5.01 4.71 4.44 4.18 3.95 3.73 3.53 3.36 3.20 3.06 2.94 2.85 2.77 2.70 2.67 2.64 2.64 2.65 2.70 2.75 2.82 2.91 3.02 3.15 3.29 3.46 3.64 3.84 4.06 4.27 4.48 4.68 4.88 5.06 5.23 5.38 5.52 5.63 5.71 5.76 5.75 5.72 5.62 5.47 5.26 5.01 4.74 4.45 4.16 3.90 3.66 3.45 3.25 3.08 2.92 2.78 2.66 2.55 2.46 2.37 2.31 2.24 2.19 2.15 2.11 2.08 2.05 2.03 2.02 2.01 </p><p><b>device</b>: <a href="DeviceMetric-CVPSampleArrayDeviceMetric.html">DeviceMetric: extension = 25 mm/s,,; type = MDC_PRESS_BLD_VEN_CENT; unit = MDC_DIM_MMHG; operationalStatus = on; color = cyan; category = measurement</a></p></div>
      </text>
      <status value="final"/>
      <code>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="150084"/>
          <display value="MDC_PRESS_BLD_VEN_CENT"/>
        </coding>
      </code>
      <subject>🔗
        <reference value="Patient/SomePatient"/>
      </subject>
      <effectivePeriod>
        <start value="2021-07-09T11:33:23+02:00"/>
        <end value="2021-07-09T11:33:24+02:00"/>
      </effectivePeriod>
      <valueSampledData>
        <origin>
          <value value="0"/>
          <unit value="mmHg"/>
          <system value="http://unitsofmeasure.org"/>
          <code value="mm[Hg]"/>
        </origin>
        <period value="8"/>
        <dimensions value="1"/>
        <data
              value="2.00 2.00 2.00 2.01 2.02 2.03 2.06 2.09 2.13 2.19 2.25 2.33 2.42 2.53 2.65 2.78 2.93 3.09 3.27 3.47 3.68 3.90 4.14 4.40 4.67 4.96 5.34 5.82 6.37 6.90 7.35 7.68 7.89 7.98 8.00 7.94 7.82 7.64 7.41 7.14 6.84 6.48 6.11 5.85 5.73 5.79 5.95 6.22 6.45 6.54 6.56 6.44 6.20 5.88 5.48 5.01 4.71 4.44 4.18 3.95 3.73 3.53 3.36 3.20 3.06 2.94 2.85 2.77 2.70 2.67 2.64 2.64 2.65 2.70 2.75 2.82 2.91 3.02 3.15 3.29 3.46 3.64 3.84 4.06 4.27 4.48 4.68 4.88 5.06 5.23 5.38 5.52 5.63 5.71 5.76 5.75 5.72 5.62 5.47 5.26 5.01 4.74 4.45 4.16 3.90 3.66 3.45 3.25 3.08 2.92 2.78 2.66 2.55 2.46 2.37 2.31 2.24 2.19 2.15 2.11 2.08 2.05 2.03 2.02 2.01"/>
      </valueSampledData>
      <device>🔗
        <reference value="DeviceMetric/CVPSampleArrayDeviceMetric"/>
      </device>
    </Observation>