# Kind of relation code system - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **Kind of relation code system**

## CodeSystem: Kind of relation code system 

| | | |
| :--- | :--- | :--- |
| *Official URL*:http://hl7.org/fhir/uv/pocd/CodeSystem/kind-of-relation | *Version*:1.0.0 | |
| * Standards status: *[Trial-use](http://hl7.org/fhir/R4/versions.html#std-process) | [Maturity Level](http://hl7.org/fhir/versions.html#maturity): 2 | *Computable Name*:Kind |

 
CodeSystem for IEEE 11073-10207 Relation/Kind. The 'pm' namespace prefix refers to the BICEPS Participant Model (pm), which is the Domain Information Model defined in IEEE 11073-10207 Service-Oriented Device Exchange Protocol Specification (BICEPS). BICEPS (Basic Integrated Clinical Environment Protocol Specification) is the XML schema representation of the IEEE 11073-10201 point-of-care medical device communication model. 

 This Code system is referenced in the content logical definition of the following value sets: 

* [Kind](ValueSet-kind-of-relation.md)



## Resource Content

```json
{
  "resourceType" : "CodeSystem",
  "id" : "kind-of-relation",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/StructureDefinition/shareablecodesystem"]
  },
  "extension" : [{
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-wg",
    "valueCode" : "dev"
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-fmm",
    "valueInteger" : 2,
    "_valueInteger" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  },
  {
    "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-standards-status",
    "valueCode" : "trial-use",
    "_valueCode" : {
      "extension" : [{
        "url" : "http://hl7.org/fhir/StructureDefinition/structuredefinition-conformance-derivedFrom",
        "valueCanonical" : "http://hl7.org/fhir/uv/pocd/ImplementationGuide/hl7.fhir.uv.pocd"
      }]
    }
  }],
  "url" : "http://hl7.org/fhir/uv/pocd/CodeSystem/kind-of-relation",
  "version" : "1.0.0",
  "name" : "Kind",
  "title" : "Kind",
  "status" : "active",
  "experimental" : false,
  "date" : "2020-05-12",
  "publisher" : "HL7 International / Devices",
  "contact" : [{
    "telecom" : [{
      "system" : "url",
      "value" : "http://www.hl7.org/Special/committees/healthcaredevices"
    }]
  }],
  "description" : "CodeSystem for IEEE 11073-10207 Relation/Kind. The 'pm' namespace prefix refers to the BICEPS Participant Model (pm), which is the Domain Information Model defined in IEEE 11073-10207 Service-Oriented Device Exchange Protocol Specification (BICEPS). BICEPS (Basic Integrated Clinical Environment Protocol Specification) is the XML schema representation of the IEEE 11073-10201 point-of-care medical device communication model.",
  "jurisdiction" : [{
    "coding" : [{
      "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
      "code" : "001"
    }]
  }],
  "caseSensitive" : false,
  "content" : "complete",
  "concept" : [{
    "code" : "Rcm",
    "display" : "Recommendation",
    "definition" : "The METRIC is a recommendation for the containment tree entries defined in ./pm:Relation/@Entries"
  },
  {
    "code" : "PS",
    "display" : "Presetting",
    "definition" : "Presetting. This METRIC is a presetting for the containment tree entries defined in ./pm:Relation/@Entries."
  },
  {
    "code" : "SST",
    "display" : "Set of summary statistics",
    "definition" : "The METRIC is part of a set of summary statistics for a sample where other METRICs that belong to the summary statistics are defined in ./pm:Relation/@Entries."
  },
  {
    "code" : "ECE",
    "display" : "Effect on containment tree entries",
    "definition" : "When changed, the METRIC has an effect on the containment tree entries defined in ./pm:Relation/@Entries. If Kind is ECE, ./pm:Relation/pm:Code SHOULD be set to classify the effect."
  },
  {
    "code" : "DCE",
    "display" : "Derived from containment tree entries",
    "definition" : "The METRIC is derived from the containment tree entries defined in ./pm:Relation/@Entries. If Kind is DCE, ./pm:Relation/pm:Code MAY be set to classify the form of derivation."
  },
  {
    "code" : "Oth",
    "display" : "Other",
    "definition" : "Relation is specified by other means, e.g., ./pm:Relation/pm:Code or extension element."
  }]
}

```
