Point-of-Care Device Implementation Guide
1.0.0 - STU 1

Point-of-Care Device Implementation Guide, published by HL7 International / Devices. This guide is not an authorized publication; it is the continuous build for version 1.0.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/HL7/uv-pocd/ and changes regularly. See the Directory of published versions

## : Rhythm Status Enumeration observation example - XML Representation

Page standards status: Informative

Raw xml | Download

    <Observation xmlns="http://hl7.org/fhir">
      <id value="RhythmStatusEnumerationObservation"/>
      <meta>
        <profile
                 value="http://hl7.org/fhir/uv/pocd/StructureDefinition/EnumerationObservation"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p class="res-header-id"><b>Generated Narrative: Observation RhythmStatusEnumerationObservation</b></p><a name="RhythmStatusEnumerationObservation"> </a><a name="hcRhythmStatusEnumerationObservation"> </a><div style="display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%"><p style="margin-bottom: 0px"/><p style="margin-bottom: 0px">Profile: <a href="StructureDefinition-EnumerationObservation.html">Enumeration Observation profile</a></p></div><p><b>status</b>: Final</p><p><b>code</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 184327}">MDC_ECG_STAT_RHY</span></p><p><b>subject</b>: <a href="Patient-SomePatient.html">John Doe  Male, DoB: 1967-05-04 ( Medical record number)</a></p><p><b>effective</b>: 2021-07-09 11:33:24+0200</p><p><b>value</b>: <span title="Codes:{urn:iso:std:iso:11073:10101 147474}">Sinus rhythm</span></p><p><b>device</b>: <a href="DeviceMetric-RhythmStatusEnumerationDeviceMetric.html">DeviceMetric: type = MDC_ECG_STAT_RHY; operationalStatus = on; category = measurement</a></p></div>
      </text>
      <status value="final"/>
      <code>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="184327"/>
          <display value="MDC_ECG_STAT_RHY"/>
        </coding>
      </code>
      <subject>🔗
        <reference value="Patient/SomePatient"/>
      </subject>
      <effectiveDateTime value="2021-07-09T11:33:24+02:00"/>
      <valueCodeableConcept>
        <coding>
          <system value="urn:iso:std:iso:11073:10101"/>
          <code value="147474"/>
          <display value="MDC_ECG_SINUS_RHY"/>
        </coding>
        <text value="Sinus rhythm"/>
      </valueCodeableConcept>
      <device>🔗
        <reference value="DeviceMetric/RhythmStatusEnumerationDeviceMetric"/>
      </device>
    </Observation>