# NBP Numeric metric example - Point-of-Care Device Implementation Guide v1.0.0

* [**Table of Contents**](toc.md)
* [**Artifact List**](artifacts.md)
* **NBP Numeric metric example**

## Example DeviceMetric: NBP Numeric metric example

| |
| :--- |
| *Page standards status:*[Informative](http://hl7.org/fhir/R4/versions.html#std-process) |

Profile: [Numeric DeviceMetric profile](StructureDefinition-NumericDeviceMetric.md)

**Metric availability extension**: intr

**type**: NBP

**unit**: mmHg

**source**: [Device: extension = ,->Practitioner Alice B. Careful ,8760,156,Dmo; identifier = urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680#01-23-45-67-89-AB-CD-EF; status = active; manufacturer = MyCompany; serialNumber = 123456; modelNumber = PM1; type = MDC_DEV_MON_PHYSIO_MULTI_PARAM_MDS](Device-PhysioMonitorMdsDevice.md)

**parent**: [Device: status = active; type = MDC_DEV_PRESS_BLD_NONINV_CHAN](Device-NBPChannelDevice.md)

**operationalStatus**: On

**color**: Color Red

**category**: Measurement

**measurementPeriod**: Once per 15 minutes



## Resource Content

```json
{
  "resourceType" : "DeviceMetric",
  "id" : "NBPNumericDeviceMetric",
  "meta" : {
    "profile" : ["http://hl7.org/fhir/uv/pocd/StructureDefinition/NumericDeviceMetric"]
  },
  "extension" : [{
    "url" : "http://hl7.org/fhir/uv/pocd/StructureDefinition/metric-availability",
    "valueCode" : "intr"
  }],
  "type" : {
    "coding" : [{
      "system" : "urn:iso:std:iso:11073:10101",
      "code" : "150020",
      "display" : "MDC_PRESS_BLD_NONINV"
    }],
    "text" : "NBP"
  },
  "unit" : {
    "coding" : [{
      "system" : "urn:iso:std:iso:11073:10101",
      "code" : "266016",
      "display" : "MDC_DIM_MMHG"
    }],
    "text" : "mmHg"
  },
  "source" : {
    "reference" : "Device/PhysioMonitorMdsDevice"
  },
  "parent" : {
    "reference" : "Device/NBPChannelDevice"
  },
  "operationalStatus" : "on",
  "color" : "red",
  "category" : "measurement",
  "measurementPeriod" : {
    "repeat" : {
      "frequency" : 1,
      "period" : 15,
      "periodUnit" : "min"
    }
  }
}

```
