HL7 v2.8.2 Vocabulary
0.2.0 - ci-build

HL7 v2.8.2 Vocabulary, published by HL7/FO. This guide is not an authorized publication; it is the continuous build for version 0.2.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/frankoemig/hl7.v2.terminology.v282/ and changes regularly. See the Directory of published versions

## CodeSystem: Remote Control Command (2.8.2 - 1.1.0) (Experimental)

Official URL: http://terminology.hl7.org/v2plusvocab/CodeSystem/remoteControlCommand | Version: 1.1.0
Active as of 2026-03-13 | Computable Name: RemoteControlCommand
Other Identifiers: OID:2.16.840.1.113883.18.226, urn:ietf:rfc:3986#Uniform Resource Identifier (URI)#http://terminology.hl7.org/v2plusvocab/CodeSystem/v2-0368
Copyright/Legal: HL7 Inc., 2026

Code system of concepts that identify the comment the component is to initiate. Used in the Equipment Command (ECD) and Interaction Status Detail (ISD) segments in HL7 Version 2.x messaging.

This Code system is referenced in the content logical definition of the following value sets:

- Hl7VSremoteControlCommand

Properties

This code system defines the following properties for its concepts

Name | Code | URI | Type | Description
version introduced | versionIntroduced | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionIntroduced | string | version when was this code introduced
version deprecated | versionDeprecated | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionDeprecated | string | version when was this code deprecated
status | status | http://hl7.org/fhir/concept-properties#status | code | A code that indicates the status of the concept. Typical values are active, experimental, deprecated, and retired
comment, to suppress IG-publisher warning, to be replaced with standard later | comment | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#comment | string | A string that provides additional detail pertinent to the use or understanding of the concept
usage | usage | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#usage | string | usage notes for this code
modified | modified | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#modified | dateTime | date of last modification

Concepts

This case-sensitive code system `http://terminology.hl7.org/v2plusvocab/CodeSystem/remoteControlCommand` defines the following codes:

Code | Display | Definition | version introduced | modified
AB | Abort | Abort | 2.4 | 2015-07-13
AF | Aliquot From container | Aliquot From container | 2.8 | 2015-07-13
AT | Aliquot To container | Aliquot To container | 2.8 | 2015-07-13
CL | Clear | Clear | 2.4 | 2015-07-13
CN | Clear Notification | Clear Notification | 2.4 | 2015-07-13
DI | Disable Sending Events | Disable Sending Events | 2.4 | 2015-07-13
EN | Enable Sending Events | Enable Sending Events | 2.4 | 2015-07-13
ES | Emergency -stop | Emergency -stop | 2.4 | 2015-07-13
EX | Execute | Execute (command specified in field Parameters (ST) 01394) | 2.4 | 2015-07-13
IN | Initialize/Initiate | Initialize/Initiate | 2.4 | 2015-07-13
LC | Local Control Request | Local Control Request | 2.4 | 2015-07-13
LK | Lock | Lock | 2.4 | 2015-07-13
LO | Load | Load | 2.4 | 2015-07-13
PA | Pause | Pause | 2.4 | 2015-07-13
RC | Remote Control Request | Remote Control Request | 2.4 | 2015-07-13
RE | Resume | Resume | 2.4 | 2015-07-13
SA | Sampling | Sampling | 2.4 | 2015-07-13
SU | Setup | Setup | 2.4 | 2015-07-13
TT | Transport To | Transport To | 2.4 | 2015-07-13
UC | Unlock | Unlock | 2.4 | 2015-07-13
UN | Unload | Unload | 2.4 | 2015-07-13