HL7 v2.9.1 Vocabulary
0.2.0 - ci-build

HL7 v2.9.1 Vocabulary, published by HL7/FO. This guide is not an authorized publication; it is the continuous build for version 0.2.0 built by the FHIR (HL7® FHIR® Standard) CI Build. This version is based on the current content of https://github.com/frankoemig/hl7.v2.terminology.v291/ and changes regularly. See the Directory of published versions

## CodeSystem: Message Error Condition Codes (2.9.1 - 1.2.0) (Experimental)

Official URL: http://terminology.hl7.org/v2plusvocab/CodeSystem/messageErrorCondition | Version: 1.2.0
Active as of 2026-03-13 | Computable Name: MessageErrorCondition
Other Identifiers: OID:2.16.840.1.113883.18.217, urn:ietf:rfc:3986#Uniform Resource Identifier (URI)#http://terminology.hl7.org/v2plusvocab/CodeSystem/v2-0357
Copyright/Legal: HL7 Inc., 2026

HL7-defined code system of concepts specifying the HL7 (communications) error code. Used in the ERR segment in HL7 Version 2.x messaging.

This Code system is referenced in the content logical definition of the following value sets:

- Hl7VSmessageErrorConditionCodes

Properties

This code system defines the following properties for its concepts

Name | Code | URI | Type | Description
version introduced | versionIntroduced | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionIntroduced | string | version when was this code introduced
version deprecated | versionDeprecated | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#versionDeprecated | string | version when was this code deprecated
status | status | http://hl7.org/fhir/concept-properties#status | code | A code that indicates the status of the concept. Typical values are active, experimental, deprecated, and retired
comment, to suppress IG-publisher warning, to be replaced with standard later | comment | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#comment | string | A string that provides additional detail pertinent to the use or understanding of the concept
usage | usage | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#usage | string | usage notes for this code
modified | modified | http://terminology.hl7.org/v2plusvocab/CodeSystem/Property#modified | dateTime | date of last modification

Concepts

This case-sensitive code system `http://terminology.hl7.org/v2plusvocab/CodeSystem/messageErrorCondition` defines the following codes:

Code | Display | Definition | version introduced | status | comment, to suppress IG-publisher warning, to be replaced with standard later | modified | Deutsch (German, de)
0 | Message accepted | Message accepted | 2.3.1 |  | Success. Optional, as the AA conveys success. Used for systems that must always return a status code. | 2015-07-13 | Nachricht akzeptiert
100 | Segment sequence error | Segment sequence error | 2.3.1 |  | Error: The message segments were not in the proper order, or required segments are missing. | 2015-07-13 | Fehler in der Segmentreihenfolge
101 | Required field missing | Required field missing | 2.3.1 |  | Error: A required field is missing from a segment | 2015-07-13 | erforderliches Feld leer
102 | Data type error | Data type error | 2.3.1 |  | Error: The field contained data of the wrong data type, e.g., an NM field contained "FOO". | 2015-07-13 | Datentypfehler
103 | Table value not found | Table value not found | 2.3.1 |  | Error: A field of data type ID or IS was compared against the corresponding table, and no match was found. | 2015-07-13 | fehlender Eintrag in der Tabelle
104 | Value too long | Value too long | 2.7 |  | Error: a value exceeded the normative length, or the length that the application is able to safely handle. | 2015-07-13 |
198 | Non-Conformant Cardinality | An error has been encountered related to HL7 message content. Message is not -conformant with the applicable specification’s (base standard, conformance profile or implementation profile) cardinality. | 2.9 |  | Error: Cardinality is listed as [0..3] and more than 3 of the identified element are present in the message. | 2022-08-25 |
199 | Other HL7 Error | Any other error with the HL7 syntax that is not captured in any of the other error codes in this set. | 2.9 |  | Error | 2022-08-25 |
200 | Unsupported message type | Unsupported message type | 2.3.1 |  | Rejection: The Message Type is not supported. | 2015-07-13 | Nachrichtentyp wird nicht unterstützt
201 | Unsupported event code | Unsupported event code | 2.3.1 |  | Rejection: The Event Code is not supported. | 2015-07-13 | Ereignis wird nicht unterstützt
202 | Unsupported processing id | Unsupported processing id | 2.3.1 |  | Rejection: The Processing ID is not supported. | 2015-07-13 | Processing-ID wird nicht unterstützt
203 | Unsupported version id | Unsupported version id | 2.3.1 |  | Rejection: The Version ID is not supported. | 2015-07-13 | Version wird nicht unterstützt
204 | Unknown key identifier | Retained for backwards compatibility only: This situation should be reported in ERR-5 (Application Error Code) using code 101 (Unknown Key Identifier) from code system HL70533. | 2.3.1 | backward | ERR-3 (HL7 Error Code) should be used to convey errors at the structural level and this is an application level error, which should be reported in ERR-5 (Application Error Code). | 2017-07-16 | Schlüsselwert nicht gefunden
205 | Duplicate key identifier | Retained for backwards compatibility only: This situation should be reported in ERR-5 (Application Error Code) using code 102 (Duplicate Key Identifier) from code system HL70533. | 2.3.1 | backward | ERR-3 (HL7 Error Code) should be used to convey errors at the structural level and this is an application level error, which should be reported in ERR-5 (Application Error Code). | 2017-07-16 | doppelter Schlüsselwert
206 | Application record locked | Retained for backwards compatibility only: This situation should be reported in ERR-5 (Application Error Code) using code 103 (Application record locked) from code system HL70533. | 2.3.1 | backward | ERR-3 (HL7 Error Code) should be used to convey errors at the structural level and this is an application level error, which should be reported in ERR-5 (Application Error Code). | 2017-07-16 | Datensatz durch Applikation gesperrt
207 | Application error | An application level error has occurred and the detail for that error is identified in ERR-5. | 2.3.1 |  | This value is used when no other value in this list is applicable and there is an application error reported in ERR-5. It is applicable when ERR-3 is required in an implementation guide. | 2017-07-25 | applikationsinterner Fehler